,Nominal Cooling Capacity (Tons)##number##general,Minimum Air Flow##hvac_air_flow##cubic_feet_per_minute,Maximum Air Flow##hvac_air_flow##cubic_feet_per_minute,Heating Type##other##,Voltage Comments##other##,Voltage##electrical_potential##volts,Overall Depth##length##inches,Overall Width##length##inches,Overall Height##length##inches,Unit Weight Value##number##general,Model##other##,Supply Air Connection Height##hvac_duct_size##inches,Supply Air Connection Width##hvac_duct_size##inches,Bottom Return Air Connection Height##hvac_duct_size##inches,Bottom Return Air Connection Width##hvac_duct_size##inches,Side Return Air Connection Height##hvac_duct_size##inches,Side Return Air Connection Width##hvac_duct_size##inches,Fan Horsepower##electrical_power##horsepower,Fan Full Load Amps##electrical_current##amperes,Maximum Overcurrent Protection##electrical_current##amperes,Minimum Circuit Amps##electrical_current##amperes
"[3TON]-[14.25""]-[AEFE3A00S1H]",3,600,1200,No Heat,120 VAC,120,28,14.25,30,80,AEFE3A00S1H,19.25,13.09,19.36,13.25,14.38,18.25,0.5,5.8,15,7.3
"[4TON]-[17.5""]-[AEFE4B00S1H]",4,1000,1600,No Heat,120 VAC,120,28,17.5,30,88,AEFE4B00S1H,19.25,16.34,19.36,16.5,14.38,18.25,0.75,8.7,15,10.9
"[5TON]-[21""]-[AEFE5C00S1H]",5,1400,2000,No Heat,120 VAC,120,28,21,30,92,AEFE5C00S1H,19.25,19.84,19.36,20,14.38,18.25,1,11.1,15,13.9
"[5TON]-[24.5""]-[AEFE5D00S1H]",5,1400,2000,No Heat,120 VAC,120,28,24.5,30,101,AEFE5D00S1H,19.25,23.34,19.36,23.5,14.38,18.25,1,11.1,15,13.9
