,Fan Drive##other##,Supply Air Flow##hvac_air_flow##cubic_feet_per_minute,Heating Type##other##,Voltage Comments##other##,Voltage##electrical_potential##volts,Coil Type##other##,Overall Depth##length##inches,Overall Width##length##inches,Overall Height##length##inches,Unit Weight Value##number##general,Model##other##,Supply Air Connection Height##hvac_duct_size##inches,Supply Air Connection Width##hvac_duct_size##inches,Return Air Connection Height##hvac_duct_size##inches,Return Air Connection Width##hvac_duct_size##inches,Water Connection Size##pipe_size##inches
[5-SPEED_PSC_MOTOR]-[800CFM]-[NO_HOT_WATER_COIL]-[240V]-[NO_HEAT]-[MXE0800N4E],5-speed PSC motor,800,No Hot Water Coil,208 VAC - 230 VAC,240,No Heat,20.5,17.5,27,69,MXE0800N4E,16,15.5,19.25,16,0.75
[5-SPEED_PSC_MOTOR]-[1200CFM]-[NO_HOT_WATER_COIL]-[240V]-[NO_HEAT]-[MXE1200N4E],5-speed PSC motor,1200,No Hot Water Coil,208 VAC - 230 VAC,240,No Heat,20.5,17.5,27,69,MXE1200N4E,16,15.5,19.25,16,0.75
[5-SPEED_PSC_MOTOR]-[1600CFM]-[NO_HOT_WATER_COIL]-[240V]-[NO_HEAT]-[MXE1600N4E],5-speed PSC motor,1600,No Hot Water Coil,208 VAC - 230 VAC,240,No Heat,20.5,21,28,74,MXE1600N4E,16,19,19.25,19.5,1
[5-SPEED_PSC_MOTOR]-[2000CFM]-[NO_HOT_WATER_COIL]-[240V]-[NO_HEAT]-[MXE2000N4E],5-speed PSC motor,2000,No Hot Water Coil,208 VAC - 230 VAC,240,No Heat,20.5,24.5,28,86,MXE2000N4E,16,22.5,19.25,23,1
[3-SPEED_PSC_MOTOR]-[800CFM]-[HOT_WATER_COIL_WITH_PUMP]-[120V]-[3_ROW_HOT_WATER_COIL]-[MXC08WPN2B],3-speed PSC motor,800,Hot Water Coil With Pump,120 VAC,120,3 Row Hot Water Coil,20.5,17.5,27,66,MXC08WPN2B,16,15.5,19.25,16,0.75
[3-SPEED_PSC_MOTOR]-[2000CFM]-[HOT_WATER_COIL_WITH_PUMP]-[120V]-[3_ROW_HOT_WATER_COIL]-[MXC2WP0N2B],3-speed PSC motor,2000,Hot Water Coil With Pump,120 VAC,120,3 Row Hot Water Coil,20.5,24.5,28,83,MXC2WP0N2B,16,22.5,19.25,23,1
[3-SPEED_PSC_MOTOR]-[800CFM]-[HOT_WATER_COIL_WITHOUT_PUMP]-[120V]-[3_ROW_HOT_WATER_COIL]-[MXC08WNN2B],3-speed PSC motor,800,Hot Water Coil Without Pump,120 VAC,120,3 Row Hot Water Coil,20.5,17.5,27,66,MXC08WNN2B,16,15.5,19.25,16,0.75
[3-SPEED_PSC_MOTOR]-[2000CFM]-[HOT_WATER_COIL_WITHOUT_PUMP]-[120V]-[3_ROW_HOT_WATER_COIL]-[MXC2WN0N2B],3-speed PSC motor,2000,Hot Water Coil Without Pump,120 VAC,120,3 Row Hot Water Coil,20.5,24.5,28,83,MXC2WN0N2B,16,22.5,19.25,23,1
[3-SPEED_PSC_MOTOR]-[800CFM]-[HOT_WATER_COIL_WITH_130F_AQUASTAT_&_PUMP]-[120V]-[3_ROW_HOT_WATER_COIL]-[MXC08APN2B],3-speed PSC motor,800,Hot Water Coil With 130F Aquastat & Pump,120 VAC,120,3 Row Hot Water Coil,20.5,17.5,27,66,MXC08APN2B,16,15.5,19.25,16,0.75
[3-SPEED_PSC_MOTOR]-[2000CFM]-[HOT_WATER_COIL_WITH_130F_AQUASTAT_&_PUMP]-[120V]-[3_ROW_HOT_WATER_COIL]-[MXC2AP0N2B],3-speed PSC motor,2000,Hot Water Coil With 130F Aquastat & Pump,120 VAC,120,3 Row Hot Water Coil,20.5,24.5,28,83,MXC2AP0N2B,16,22.5,19.25,23,1
[3-SPEED_PSC_MOTOR]-[800CFM]-[HOT_WATER_COIL_WITH_130F_AQUASTAT_&_WITHOUT_PUMP]-[120V]-[3_ROW_HOT_WATER_COIL]-[MXC08ANN2B],3-speed PSC motor,800,Hot Water Coil With 130F Aquastat & Without Pump,120 VAC,120,3 Row Hot Water Coil,20.5,17.5,27,66,MXC08ANN2B,16,15.5,19.25,16,0.75
[3-SPEED_PSC_MOTOR]-[2000CFM]-[HOT_WATER_COIL_WITH_130F_AQUASTAT_&_WITHOUT_PUMP]-[120V]-[3_ROW_HOT_WATER_COIL]-[MXC2AN0N2B],3-speed PSC motor,2000,Hot Water Coil With 130F Aquastat & Without Pump,120 VAC,120,3 Row Hot Water Coil,20.5,24.5,28,83,MXC2AN0N2B,16,22.5,19.25,23,1
[3-SPEED_PSC_MOTOR]-[800CFM]-[HOT_WATER_COIL_WITH_PUMP]-[120V]-[4_ROW_HOT_WATER_COIL]-[MXC08WPN2C],3-speed PSC motor,800,Hot Water Coil With Pump,120 VAC,120,4 Row Hot Water Coil,20.5,17.5,27,66,MXC08WPN2C,16,15.5,19.25,16,0.75
[3-SPEED_PSC_MOTOR]-[1200CFM]-[HOT_WATER_COIL_WITH_PUMP]-[120V]-[4_ROW_HOT_WATER_COIL]-[MXC12WPN2C],3-speed PSC motor,1200,Hot Water Coil With Pump,120 VAC,120,4 Row Hot Water Coil,20.5,17.5,27,66,MXC12WPN2C,16,15.5,19.25,16,0.75
[3-SPEED_PSC_MOTOR]-[1600CFM]-[HOT_WATER_COIL_WITH_PUMP]-[120V]-[4_ROW_HOT_WATER_COIL]-[MXC16WPN2C],3-speed PSC motor,1600,Hot Water Coil With Pump,120 VAC,120,4 Row Hot Water Coil,20.5,21,28,71,MXC16WPN2C,16,19,19.25,19.5,1
[3-SPEED_PSC_MOTOR]-[800CFM]-[HOT_WATER_COIL_WITHOUT_PUMP]-[120V]-[4_ROW_HOT_WATER_COIL]-[MXC08WNN2C],3-speed PSC motor,800,Hot Water Coil Without Pump,120 VAC,120,4 Row Hot Water Coil,20.5,17.5,27,66,MXC08WNN2C,16,15.5,19.25,16,0.75
[3-SPEED_PSC_MOTOR]-[1200CFM]-[HOT_WATER_COIL_WITHOUT_PUMP]-[120V]-[4_ROW_HOT_WATER_COIL]-[MXC12WNN2C],3-speed PSC motor,1200,Hot Water Coil Without Pump,120 VAC,120,4 Row Hot Water Coil,20.5,17.5,27,66,MXC12WNN2C,16,15.5,19.25,16,0.75
[3-SPEED_PSC_MOTOR]-[1600CFM]-[HOT_WATER_COIL_WITHOUT_PUMP]-[120V]-[4_ROW_HOT_WATER_COIL]-[MXC16WNN2C],3-speed PSC motor,1600,Hot Water Coil Without Pump,120 VAC,120,4 Row Hot Water Coil,20.5,21,28,71,MXC16WNN2C,16,19,19.25,19.5,1
[3-SPEED_PSC_MOTOR]-[800CFM]-[HOT_WATER_COIL_WITH_130F_AQUASTAT_&_PUMP]-[120V]-[4_ROW_HOT_WATER_COIL]-[MXC08APN2C],3-speed PSC motor,800,Hot Water Coil With 130F Aquastat & Pump,120 VAC,120,4 Row Hot Water Coil,20.5,17.5,27,66,MXC08APN2C,16,15.5,19.25,16,0.75
[3-SPEED_PSC_MOTOR]-[1200CFM]-[HOT_WATER_COIL_WITH_130F_AQUASTAT_&_PUMP]-[120V]-[4_ROW_HOT_WATER_COIL]-[MXC12APN2C],3-speed PSC motor,1200,Hot Water Coil With 130F Aquastat & Pump,120 VAC,120,4 Row Hot Water Coil,20.5,17.5,27,66,MXC12APN2C,16,15.5,19.25,16,0.75
[3-SPEED_PSC_MOTOR]-[1600CFM]-[HOT_WATER_COIL_WITH_130F_AQUASTAT_&_PUMP]-[120V]-[4_ROW_HOT_WATER_COIL]-[MXC16APN2C],3-speed PSC motor,1600,Hot Water Coil With 130F Aquastat & Pump,120 VAC,120,4 Row Hot Water Coil,20.5,21,28,71,MXC16APN2C,16,19,19.25,19.5,1
[3-SPEED_PSC_MOTOR]-[800CFM]-[HOT_WATER_COIL_WITH_130F_AQUASTAT_&_WITHOUT_PUMP]-[120V]-[4_ROW_HOT_WATER_COIL]-[MXC08ANN2C],3-speed PSC motor,800,Hot Water Coil With 130F Aquastat & Without Pump,120 VAC,120,4 Row Hot Water Coil,20.5,17.5,27,66,MXC08ANN2C,16,15.5,19.25,16,0.75
[3-SPEED_PSC_MOTOR]-[1200CFM]-[HOT_WATER_COIL_WITH_130F_AQUASTAT_&_WITHOUT_PUMP]-[120V]-[4_ROW_HOT_WATER_COIL]-[MXC12ANN2C],3-speed PSC motor,1200,Hot Water Coil With 130F Aquastat & Without Pump,120 VAC,120,4 Row Hot Water Coil,20.5,17.5,27,66,MXC12ANN2C,16,15.5,19.25,16,0.75
[3-SPEED_PSC_MOTOR]-[1600CFM]-[HOT_WATER_COIL_WITH_130F_AQUASTAT_&_WITHOUT_PUMP]-[120V]-[4_ROW_HOT_WATER_COIL]-[MXC16ANN2C],3-speed PSC motor,1600,Hot Water Coil With 130F Aquastat & Without Pump,120 VAC,120,4 Row Hot Water Coil,20.5,21,28,71,MXC16ANN2C,16,19,19.25,19.5,1
