{"text_format":"1","workbook":"xlsx","n_sheets":45,"sheets":["Prompt","Instructions","Form","HPRatings","ACRatings","OutdoorUnitData","outdoor-images","IndoorUnitData","indoor-images","dimensions-images","Options","Schedule","HP-Report","AC-Report","Indoor-Report","AM-Dimension","AV-Dimension","AX-Dimension","THGD_YORK_SUMMARY","YHJD_YORK_SUMMARY","YHM_YORK_SUMMARY","HMH_YORK_SUMMARY","THE_YORK_SUMMARY","YHE_YORK_SUMMARY","YH2E_YORK_SUMMARY","YH2F_YORK_SUMMARY","YEE_YORK_SUMMARY","YHG_YORK_SUMMARY","YZT_YORK_SUMMARY","YHJF_YORK_SUMMARY","YHJR_YORK_SUMMARY","YZF_YORK_SUMMARY","YZH_YORK_SUMMARY","YCJF_YORK_SUMMARY","YZV_YORK_SUMMARY","YH4_YORK_SUMMARY","HH8_YORK_SUMMARY","YH6_YORK_SUMMARY","YH5_YORK_SUMMARY","OD_SUMMARY","AM_SUMMARY","AV_SUMMARY","AX_SUMMARY","ID_SUMMARY","Print"],"not_rendered":{"charts":0,"images":52,"macros":1,"external_links":0,"defined_names":34,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Prompt","index":0,"n_rows":17,"n_cols":1,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
["Confidential & Proprietary ADP Information for USACD Use Only"]
[]
[]
[]
[]
["In order to use this spreadsheet, "]
["Please enable Macros in your security settings."]
[]
["Enabling Macros in Excel 2007"]
["1. In Excel, click the Office button in the upper left corner of the screen."]
["2. Click the \"Excel Options\" button in the lower right."]
["3. Click the \"Trust Center\" button on the left. Then, at the bottom right, select \"Trust Center Settings\" as shown below."]
["4. In the next window, select \"Macro Settings,\" then select the radio button for \"Disable all macros with notification.\""]
["5. When opening this spreadsheet, you will see a warning like this in the menu bar:"]
[]
[]
["6. Select \"Enable this content\" and click \"Okay\".  The spreadsheet will now be functional."]

{"sheet":"Instructions","index":1,"n_rows":39,"n_cols":3,"rows_kept":39,"cut":false,"hidden":false,"merged":[[8,0,10,4],[14,0,17,4],[18,0,18,4],[25,0,25,4],[0,0,0,4],[3,0,3,4],[4,0,6,4],[12,0,12,4],[11,0,11,4],[20,0,20,4],[21,0,21,4],[23,0,23,4],[22,0,22,4],[1,0,2,4],[36,0,36,4],[33,0,33,4],[34,0,34,4],[35,0,35,4],[26,0,27,4],[29,0,29,4],[31,0,31,4],[30,0,30,4]]}
["Confidential & Proprietary ADP Information for USACD Use Only"]
[]
[]
[]
["This spreadsheet generates match-up listings for ADP indoor units with air conditioners and heat pumps at AHRI standard conditions.  The user selects nominal tonnages and SEER ranges for printing of related data and dimension sheets."]
[]
[]
[]
["•   The information provided is not certified and is for engineering use only. \n•   The latest version is available at:  www.adpnow.com/USACD\n•   In order to develop a selection, you will need the following information:"]
[]
[]
["Nominal tonnage\nSEER range"]
["SEER range"]
[]
["•   Enter the desired Project Name to be printed on the data and dimension sheets.\n•   Enter the desired Unit Tag to be printed on the data and dimension sheets.\n•   Select the Nominal Tonnage from the drop down list.\n•   Enter the desired SEER Range minimum and maximum values.  Note the limits of values allowed."]
[]
[]
[]
["Click on \"Search\" to list all AHRI numbers that meet the entered tonnage and SEER range."]
[]
["The table can be sorted and filtered using the arrows in each column (e.g. OEM Name, SEER, EER, etc.)         \nFrom this point you may:"]
["From this point you may:"]
["Click \"Clear\" to clear the form and start over.\nClick any number of selection boxes on the Form to add these match-ups to the Schedule."]
["Click any number of selection boxes on the Form to add these match-ups to the Schedule."]
[]
["When  satisfied with the selections, click \"Add to Schedule\" to display the Schedule tab.\n"]
["You may filter and sort selections in the Schedule or select one with a radio button to generate a report."]
[]
[]
["Click \"Reports\" to generate three report tabs -- outdoor,  indoor, and indoor dimensions."]
["Click \"Print\" to print a copy of the reports."]
["Click \"Save as PDF\" to save the reports to a file."]
[]
["Notes:"]
["Indoor unit data includes air flow & static pressures."]
["Dimensions, weights, utility requirements and general information are provided on report tabs."]
["See distributor for additional information."]
[]
["Version:    ","USACD-25-B","2025-08-25"]

{"sheet":"Form","index":2,"n_rows":11,"n_cols":19,"rows_kept":11,"cut":false,"hidden":false,"merged":[[7,8,7,9],[8,8,8,11],[3,8,3,11],[1,1,1,13],[2,8,2,11],[4,8,4,9],[5,8,5,9],[6,8,6,9],[2,3,2,5]]}
[]
[null,"Confidential & Proprietary ADP Information for USACD Use Only"]
[null,null,"Project Name:  ",null,null,null,null,null,"Cooling Data"]
[null,null,"Engineer:  ",null,"Contractor: "]
[null,null,"Unit Tag:  ",null,"Quantity: ",null,null,null,"Outdoor Dry Bulb:",null,95,"(°F) "]
[null,null,"Nominal Tonnage:  ",null,null,null,null,null,"Entering Dry Bulb:","Entering Dry Bulb:",80,"(°F) "]
[null,null,"SEER2 Range:  ",null," (min) 13",null," (max) 19",null,"Entering Wet Bulb:","Entering Wet Bulb:",67,"(°F) "]
[]
[]
[]
[null," ","AHRI Number","OEM Name","Outside Model","Inside Model","Capacity2 95°F","SEER2","EER2","Airflow","Capacity2 47°F","HSPF2","Capacity2 17°F","Metering Device","Min Circuit Ampacity","Max Over-current Protection","Compressor Type","Multi-stage Compressor","Power Supply"]

{"sheet":"HPRatings","index":3,"n_rows":101,"n_cols":16,"rows_kept":101,"cut":false,"hidden":true,"merged":[]}
["AHRI Reference Number","OEM Name","Outdoor Model","Indoor Model","Refrigerant","Capacity2 95°F","EER2","SEER2","Airflow","Capacity2 47°F","HSPF2","Capacity2 17°F","Metering Device Type","Metering device","Factory Installed","Tonnage"]
[202349386,"YORK","YZT36B21","AV360CT","R-410A",34000,13,17,1175,33400,7.5,22200,"TXV","165616601A","Factory",3]
[206842434,"YORK","HMH72B361","AX361CT","R-410A",35600,8.5,17,1175,34400,8.4,23000,"TXV","165616601A","Factory",3]
[216019509,"YORK","YH2E60TB21","AX600C*C+TXV","R-410A",54500,11,14.5,1775,52000,7.5,33800,"TXV","165616602A","Field",5]
[209551790,"YORK","YZT48B21","AX480CT","R-410A",47500,12,17,1600,45000,8,29200,"TXV","165616602A","Factory",4]
[207769451,"YORK","HMH72B601","AX601CT","R-410A",58000,8,16,1550,55000,7.8,34800,"TXV","165616602A","Factory",5]
[215876540,"YORK","YH436E2S11","AX360C*A+TXV","R-454B",33400,11,14.3,1175,30000,7.5,19200,"TXV","167757901A","Field",3]
[211719659,"YORK","YH2E18SB21","AX182ATA","R-410A",16900,12,14.5,600,14800,7.5,8200,"TXV","165616601A","Factory",1.5]
[211310353,"YORK","YH2F30TB21","AX360CTA","R-410A",29800,11.7,17,1000,27000,7.8,16800,"TXV","165616601A","Factory",3]
[211627121,"YORK","YZT36B21","AX360CTA","R-410A",33800,12.5,16,1175,33400,7.5,22200,"TXV","165616601A","Factory",3]
[211302363,"YORK","HMH72B481","AX482CTA","R-410A",48000,10,17,1500,45500,7.8,27800,"TXV","165616602A","Factory",4]
[215876542,"YORK","YH536E2S11","AX362C*A+TXV","R-454B",32400,11,15.2,1200,30200,8.1,19400,"TXV","167757901A","Field",3]
[209551794,"YORK","YZT60B21","AX601CT","R-410A",54500,12,15.2,1600,57000,7.8,40000,"TXV","165616602A","Factory",5]
[202363965,"YORK","YZT60B21","AX602CT","R-410A",55000,12.5,15.2,1600,57000,7.8,40000,"TXV","165616602A","Factory",5]
[206842436,"YORK","HMH72B601","AX602CT","R-410A",58500,8.5,17,1550,55000,7.8,34800,"TXV","165616602A","Factory",5]
[207768711,"YORK","HMH72B481","AX600CT","R-410A",48000,10,17,1500,45500,7.8,27800,"TXV","165616602A","Factory",5]
[215876547,"YORK","YH560E2S11","AX600C*C+TXV","R-454B",55500,11.7,14.5,1650,54500,7.8,36800,"TXV","167757902A","Field",5]
[215438159,"YORK","HH824E2S11","AX241B*C+TXV","R-454B",23600,11.7,19,775,22400,9.25,16800,"TXV","167757901A","Field",2]
[211302361,"YORK","YH2E48TB21","AX482CTA","R-410A",47000,10.5,14.5,1500,46500,7.7,30800,"TXV","165616602A","Factory",4]
[216019506,"YORK","HMH72B601","AX600C*C+TXV","R-410A",57000,8,16,1600,54000,8.25,35000,"TXV","165616602A","Field",5]
[207093915,"YORK","HMH72B361","AV360CT","R-410A",36000,9,18,1175,34400,8.5,23000,"TXV","165616601A","Factory",3]
[211286019,"YORK","YH2F18SB21","AX242BTA","R-410A",17600,12.2,15.2,750,16000,7.8,11800,"TXV","165616601A","Factory",2]
[211286021,"YORK","YH2F36TB21","AX362CTA","R-410A",34600,11.7,15.2,1200,32600,7.8,20200,"TXV","165616601A","Factory",3]
[210797899,"YORK","YH2F24TB21","AX241BT","R-410A",22800,11,14.3,750,20000,7.6,12500,"TXV","165616601A","Factory",2]
[202349339,"YORK","YZT24B21","AX240BT","R-410A",22400,12.5,17,800,21000,7.6,14000,"TXV","165616601A","Factory",2]
[211257272,"YORK","YH2E60TB21","AX600CT","R-410A",54500,11,14.3,1850,54500,7.5,35800,"TXV","165616602A","Factory",5]
[211286018,"YORK","YH2E42TB21","AX422CTA","R-410A",40000,11,14.3,1325,39000,7.5,25000,"TXV","165616602A","Factory",3.5]
[216019524,"YORK","HH860E2S11","AX600CT","R-454B",46000,12,19,1550,44000,9,34000,"TXV","167757902A","Factory",5]
[207768713,"YORK","HMH72B481","AX601CT","R-410A",48000,10,17,1500,45500,7.8,27800,"TXV","165616602A","Factory",5]
[216751172,"YORK","YH448E2S11","AX482C*A+TXV","R-454B",47000,11,15,1600,45000,7.5,28400,"TXV","167757902A","Field",4]
[214094708,"YORK","YH2E30TB21","AX360CTA","R-410A",29200,11,15,950,26000,7.5,15300,"TXV","165616601A","Factory",3]
[205765787,"YORK","YZT24B21","AX300CT","R-410A",24000,13.5,19,800,21600,7.55,12900,"TXV","165616601A","Factory",2.5]
[215876544,"YORK","YH536E2S11","AX361C*C+TXV","R-454B",32800,11,15,1200,30000,7.75,19400,"TXV","167757901A","Field",3]
[215876546,"YORK","YH548E2S11","AX482C*A+TXV","R-454B",47000,12,14.5,1600,44000,8.1,29800,"TXV","167757902A","Field",4]
[211286017,"YORK","YH2E24TB21","AX242BTA","R-410A",23600,11,14.5,800,20400,7.5,13800,"TXV","165616601A","Factory",2]
[211286016,"YORK","YH2E30TB21","AX362CTA","R-410A",29200,11,15,950,27600,7.5,16900,"TXV","165616601A","Factory",3]
[211756657,"YORK","HMH72B241","AX242BTA","R-410A",21200,9.5,17,750,21000,7.8,13400,"TXV","165616601A","Factory",2]
[215438151,"YORK","HH860E2S11","AV480C*+TXV","R-454B",44500,11.7,18,1450,42500,8.9,31600,"TXV","167757902A","Field",4]
[211310173,"YORK","HMH72B361","AX360CTA","R-410A",36000,9,18,1175,34400,8.5,23000,"TXV","165616601A","Factory",3]
[207573349,"YORK","HMH72B601","AV600CT","R-410A",58000,8,16,1550,55000,7.8,34800,"TXV","165616602A","Factory",5]
[210797902,"YORK","YH2F36TB21","AX361CT","R-410A",34200,11.5,15,1200,32600,7.7,20200,"TXV","165616601A","Factory",3]
[211310355,"YORK","YH2F36TB21","AX360CTA","R-410A",35000,12,15,1175,31800,7.8,22200,"TXV","165616601A","Factory",3]
[211627123,"YORK","HMH72B341","AX362CTA","R-410A",34000,10.5,18,1200,33400,9.6999999999999993,23000,"TXV","165616601A","Factory",3]
[202364779,"YORK","YZT48B21","AX602CT","R-410A",47500,12,17,1600,45000,7.95,28600,"TXV","165616602A","Factory",5]
[207093916,"YORK","HMH72B361","AX360CT","R-410A",36000,9,18,1175,34400,8.5,23000,"TXV","165616601A","Factory",3]
[215438148,"YORK","HH836E2S11","AX362C*A+TXV","R-454B",33800,11.7,19,1150,29400,8.5,25600,"TXV","167757901A","Field",3]
[215438150,"YORK","HH836E2S11","AX361C*C+TXV","R-454B",33400,11.5,18,1150,29400,8.4,25600,"TXV","167757901A","Field",3]
[211627122,"YORK","YZT48B21","AX482CTA","R-410A",47500,12.5,18,1600,45000,8.0500000000000007,29200,"TXV","165616602A","Factory",4]
[209551791,"YORK","YZT48B21","AV600CT","R-410A",46500,11.5,15,1600,45000,7.9,28600,"TXV","165616602A","Factory",5]
[206842435,"YORK","HMH72B481","AX602CT","R-410A",48000,10,17,1500,45500,7.8,27800,"TXV","165616602A","Factory",5]
[215876541,"YORK","YH460E2S11","AX600C*C+TXV","R-454B",54500,11,15,1825,56000,7.5,36400,"TXV","167757902A","Field",5]
[215876543,"YORK","YH536E2S11","AX360C*A+TXV","R-454B",33600,11.7,15.2,1175,30000,8.1,19000,"TXV","167757901A","Field",3]
[211286020,"YORK","YH2F30TB21","AX362CTA","R-410A",29400,11.7,16,950,25800,7.8,18000,"TXV","165616601A","Factory",3]
[216751171,"YORK","YH518E2S11","AX182A*A+TXV","R-454B",16900,12,16,600,14900,7.55,9400,"TXV","167757901A","Field",1.5]
[211286013,"YORK","YH2E36TB21","AX362CTA","R-410A",35000,10.5,14.5,1250,32400,7.5,22000,"TXV","165616601A","Factory",3]
[211627120,"YORK","YZT36B21","AX362CTA","R-410A",33400,12,15.2,1200,32800,7.6,20800,"TXV","165616601A","Factory",3]
[207573348,"YORK","HMH72B481","AV600CT","R-410A",48000,10,17,1575,46000,7.8,28200,"TXV","165616602A","Factory",5]
[215438153,"YORK","HH860E2S11","AX480C*C+TXV","R-454B",46000,12,18,1550,44000,9,34000,"TXV","167757902A","Field",4]
[211627124,"YORK","HMH72B341","AX360CTA","R-410A",34000,10.5,18,1200,33400,9.6999999999999993,23000,"TXV","165616601A","Factory",3]
[211291589,"YORK","HMH72B361","AX362CTA","R-410A",36000,9,18,1175,34400,8.5,23000,"TXV","165616601A","Factory",3]
[213743900,"YORK","YH2F42TB21","AV480CT","R-410A",40500,11.7,15.2,1350,36800,8,23400,"TXV","165616602A","Factory",4]
[216019519,"YORK","YH460E2S11","AX600CT","R-454B",55000,11,15,1850,55500,7.5,36400,"TXV","167757902A","Factory",5]
[216797738,"YORK","HH824E2S11","AX241A*C+TXV","R-454B",23800,11.7,19,775,22400,9.25,16800,"TXV","167757901A","Field",2]
[215876545,"YORK","YH548E2S11","AV480C*+TXV","R-454B",45000,11.5,14.5,1450,43500,7.7,27800,"TXV","167757902A","Field",4]
[211302362,"YORK","YH2F48TB21","AX482CTA","R-410A",46500,12,15.2,1500,42000,8.1,27800,"TXV","165616602A","Factory",4]
[215438160,"YORK","HH824E2S11","AX242B*A+TXV","R-454B",24000,12,19,775,22400,9.5,16800,"TXV","167757901A","Field",2]
[202346024,"YORK","YZT36B21","AX360CT","R-410A",33800,12.5,16,1175,33400,7.5,22200,"TXV","165616601A","Factory",3]
[210797901,"YORK","YH2F30TB21","AX361CT","R-410A",28800,11.5,16,1000,26800,7.65,16800,"TXV","165616601A","Factory",3]
[210908557,"YORK","YH2F48TB21","AV480CT","R-410A",45000,10.5,15,1500,43000,7.5,29600,"TXV","165616602A","Factory",4]
[211627126,"YORK","HMH72B481","AV480CT","R-410A",46000,9.5,17,1500,46000,7.5,28200,"TXV","165616602A","Factory",4]
[216019511,"YORK","YZT60B21","AX600C*C+TXV","R-410A",54000,12,15.2,1600,57000,7.75,40000,"TXV","165616602A","Field",5]
[211286024,"YORK","YH2F24TB21","AX242BTA","R-410A",23600,11.7,15.2,750,20000,7.8,12500,"TXV","165616601A","Factory",2]
[216019521,"YORK","YH560E2S11","AX600CT","R-454B",55500,11,16,1850,55000,7.8,36400,"TXV","167757902A","Factory",5]
[212361497,"YORK","YZT24B21","AX242BTA","R-410A",22200,12.5,17,800,20800,7.5,13900,"TXV","165616601A","Factory",2]
[211756656,"YORK","HMH72B241","AX241BT","R-410A",20400,9,15.2,750,21000,7.6,13400,"TXV","165616601A","Factory",2]
[208101085,"YORK","YZT60B21","AV600CT","R-410A",54500,12,14.5,1600,57000,7.8,40000,"TXV","165616602A","Factory",5]
[209551788,"YORK","YZT48B21","AX600CT","R-410A",47000,11.5,17,1600,45000,7.85,28600,"TXV","165616602A","Factory",5]
[215876538,"YORK","YH424E2S11","AX242B*A+TXV","R-454B",23600,11,14.3,800,20800,7.5,12900,"TXV","167757901A","Field",2]
[215438152,"YORK","HH860E2S11","AX600C*C+TXV","R-454B",53500,12,18,1625,51500,8.5,35200,"TXV","167757902A","Field",5]
[215438154,"YORK","HH860E2S11","AX482C*A+TXV","R-454B",46000,12,18,1550,44000,9,34000,"TXV","167757902A","Field",4]
[210797904,"YORK","YH2F60TB21","AX600CT","R-410A",56000,11.7,16,1650,56000,8.1,37600,"TXV","165616602A","Factory",5]
[211286025,"YORK","YH2F42TB21","AX422CTA","R-410A",41000,12.2,15.2,1325,40500,8.1,28400,"TXV","165616602A","Factory",3.5]
[216019514,"YORK","YH2F60TB21","AX600C*C+TXV","R-410A",56000,12,16,1750,54000,8.1,36200,"TXV","165616602A","Field",5]
[215876539,"YORK","YH524E2S11","AX242B*A+TXV","R-454B",24000,12,15.2,800,21200,7.8,12800,"TXV","167757901A","Field",2]
[206842433,"YORK","HMH72B241","AX240BT","R-410A",21200,9.5,17,750,21000,7.8,13400,"TXV","165616601A","Factory",2]
[212361607,"YORK","YZT60B21","AX600CT","R-410A",54000,12,15.2,1600,57000,7.75,40000,"TXV","165616602A","Factory",5]
[211627125,"YORK","HMH72B341","AX361CT","R-410A",33600,9.5,18,1200,37400,8.4,23800,"TXV","165616601A","Factory",3]
[210908426,"YORK","YH2E42TB21","AV480CT","R-410A",40000,11,14.3,1325,39000,7.5,25000,"TXV","165616602A","Factory",5]
[215438149,"YORK","HH836E2S11","AX360C*A+TXV","R-454B",33400,11.7,19,1175,29400,9,24200,"TXV","167757901A","Field",3]
[207768712,"YORK","HMH72B481","AX480CT","R-410A",48000,10,17,1575,46000,7.8,28200,"TXV","165616602A","Factory",4]
[209551793,"YORK","YZT48B21","AX601CT","R-410A",47500,12,17,1600,45000,7.9,28600,"TXV","165616602A","Factory",4]
[217197802,"YORK","YH648E2S11","AX482C*A+TXV","R-454B",48000,12,16,1600,44500,8.1,31200,"TXV","167757902A","Factory",4]
[217197803,"YORK","YH660E2S11","AX600C*C+TXV","R-454B",55000,12,16,1775,55000,8.1,37400,"TXV","167828102A","Factory",5]
[217197811,"YORK","YH624E2S11","AX241A*C+TXV","R-454B",22800,11.5,14.5,800,21600,7.8,14100,"TXV","167828101A ","Factory",2]
[217197812,"YORK","YH624E2S11","AX242B*A+TXV","R-454B",23600,12,16,800,21600,8,14100,"TXV","167757901A","Factory",2]
[217197813,"YORK","YH636E2S11","AX362C*A+TXV","R-454B",34000,12,16,1150,32800,8.1,21400,"TXV","167757901A","Factory",3]
[217197814,"YORK","YH636E2S11","AX360C*A+TXV","R-454B",35200,12,16,1175,33800,8.1,21600,"TXV","167757901A","Factory",3]
[217197815,"YORK","YH636E2S11","AX361C*C+TXV","R-454B",33000,11.5,16,900,34000,7.95,22000,"TXV","167828101A ","Factory",3]
[217549971,"YORK","YH648E2S11","AX600C*A+TXV","R-454B",48000,12,16.899999999999999,1600,44500,8.1,31200,"TXV","167757902A","Factory",4]
[217549972,"YORK","YH648E2S11","AX480C*A+TXV","R-454B",48000,12,16,1600,44500,8.1,31200,"TXV","167757902A","Factory",4]
[217735898,"YORK","YH660E2S11","AX600C*A+TXV","R-454B",55000,12,16,1775,55000,8.1,37400,"TXV","167757902A","Factory",5]

{"sheet":"ACRatings","index":4,"n_rows":1,"n_cols":12,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["AHRI Reference Number","OEM Name","Outdoor Model","Indoor Model","Refrigerant","Capacity 95°F","EER","SEER","Airflow","Metering Device Type","Metering Device","Factory Installed"]

{"sheet":"OutdoorUnitData","index":5,"n_rows":142,"n_cols":15,"rows_kept":142,"cut":false,"hidden":true,"merged":[]}
["OUTDOOR MODEL","POWER SUPPLY","MIN CIRCUIT AMPACITY","MAX OVER-CURRENT PROTECTION","COMPRESSOR TYPE","MULTI-STAGE COMPRESSOR","MOTOR R.L.A. @ 230 V","COMPRESSOR R.L.A. @ 230 V","COMPRESSOR L.R.A @ 230 V","TOTAL F.L.A. @ 230 V","NOMINAL AIR FLOW (CFM)","HEIGHT","DEPTH","WIDTH","WEIGHT (lbs.)"]
["YHE18B21","208/230 1-60",12,20,"Scroll","No",0.8,9,56.3,9.8000000000000007,2850,"33.25\"","29.25\"","29.25\"",120]
["YHE24B21","208/230 1-60",15.4,25,"Scroll","No",0.8,11.7,61.6,12.5,2850,"36.25\"","29.25\"","29.25\"",131]
["YHE30B21","208/230 1-60",18.100000000000001,30,"Scroll","No",1.3,13.4,72.5,14.7,2995,"39.5\"","35.25\"","31.75\"",176]
["YHE35B21","208/230 1-60",20.5,35,"Scroll","No",1.3,15.4,83.9,16.7,2995,"39.5\"","35.25\"","31.75\"",176]
["YHE36B21","208/230 1-60",19.7,30,"Recip","No",1.3,14.7,78,16,3715,"39.5\"","35.25\"","31.75\"",230]
["YHE36B22","208/230 1-60",21.99,35,"Scroll","No",2.8,15.35,83.9,18.2,3715,"39.5\"","38\"","34.25\"",200]
["YHE42B21","208/230 1-60",25.5,40,"Recip","No",1.3,19.399999999999999,88,20.7,3715,"39.5\"","35.25\"","31.75\"",230]
["YHE42B22","208/230 1-60",25.5,40,"Recip","No",1.3,19.399999999999999,88,20.7,3715,"39.5\"","35.25\"","31.75\"",230]
["YHE42B23","208/230 1-60",25.5,40,"Recip","No",1.3,19.399999999999999,88,20.7,3715,"39.5\"","35.25\"","31.75\"",230]
["YHE48B21","208/230 1-60",30.8,50,"Scroll","No",1.3,23.6,130,24.9,4000,"39.5\"","38\"","31.75\"",235]
["YHE48B22","208/230 1-60",30.8,50,"Scroll","No",1.3,23.6,130,24.9,4000,"39.5\"","38\"","34.25\"",235]
["YHE60B21","208/230 1-60",31.7,50,"Scroll","No",1.3,24.3,144.19999999999999,25.6,4100,"42.75\"","38\"","34.25\"",256]
["YHE60B22","208/230 1-60",31.7,50,"Scroll","No",1.3,24.3,144.19999999999999,25.6,4100,"42.75\"","38\"","34.25\"",256]
["YHJD18S41S7","208/230 1-60",11.9,20,"Scroll","No",0.7,9,48,9.6999999999999993,2000,"28.25\"","34\"","34\"",172]
["YHJD24S41S7","208/230 1-60",11.2,15,"Recip","No",0.8,8.3000000000000007,43,9.1000000000000014,2900,"32.25\"","34\"","34\"",194]
["YHJD30S41S7","208/230 1-60",14.1,20,"Recip","No",1.3,10.6,54,11.9,3800,"36.25\"","34\"","34\"",206]
["YHJD30S43S3","208/230 3-60",11,15,"Recip","No",0.8,8.1,63,8.9,3100,"36.25\"","34\"","34\"",196]
["YHJD30S43S4","208/230 3-60",11,15,"Recip","No",0.8,8.1,63,8.9,3100,"36.25\"","34\"","34\"",196]
["YHJD30S44S3","460 3-60",6,15,"Recip","No",0.8,4.2,30,5,3100,"36.25\"","34\"","34\"",196]
["YHJD30S44S4","460 3-60",6,15,"Recip","No",0.8,4.2,30,5,3100,"36.25\"","34\"","34\"",196]
["YHJD36S41S7","208/230 1-60",19.7,30,"Recip","No",1.3,14.7,74,16,3800,"40.25\"","34\"","34\"",218]
["YHJD36S43S3","208/230 3-60",12.9,20,"Recip","No",1.5,9.1,68,10.6,3800,"40.25\"","34\"","34\"",208]
["YHJD36S43S4","208/230 3-60",12.9,20,"Recip","No",1.3,9.1,68,10.4,3800,"40.25\"","34\"","34\"",208]
["YHJD36S44S3","460 3-60",6.4,15,"Recip","No",0.8,4.5,34,5.3,3800,"40.25\"","34\"","34\"",208]
["YHJD36S44S4","460 3-60",7,15,"Recip","No",0.8,4.5,34,5.3,3800,"40.25\"","34\"","34\"",208]
["YHJD42S41S7","208/230 1-60",20.9,35,"Recip","No",1.3,15.7,88,17,3800,"40.25\"","34\"","34\"",218]
["YHJD42S43S3","208/230 3-60",19.100000000000001,30,"Scroll","No",1.5,14.1,95,15.6,3800,"40.25\"","34\"","34\"",208]
["YHJD42S43S4","208/230 3-60",12.9,20,"Recip","No",1.3,12.9,68,14.200000000000001,3800,"40.25\"","34\"","34\"",208]
["YHJD42S44S3","460 3-60",8.6999999999999993,15,"Scroll","No",0.8,6.4,45,7.2,3800,"40.25\"","34\"","34\"",208]
["YHJD42S44S4","460 3-60",7.2,15,"Recip","No",0.8,5.0999999999999996,34,5.8999999999999995,3800,"40.25\"","34\"","34\"",208]
["YHJD48S41S7","208/230 1-60",20.9,35,"Recip","No",1.3,15.7,84,17,3600,"40.25\"","34\"","34\"",285]
["YHJD48S43S3","208/230 3-60",15.5,25,"Recip","No",1.3,11.2,88,12.5,3800,"40.25\"","34\"","34\"",248]
["YHJD48S44S3","460 3-60",7.2,15,"Recip","No",0.8,5.0999999999999996,44,5.8999999999999995,3800,"40.25\"","34\"","34\"",248]
["YHJD60S41S7","208/230 1-60",33,60,"Scroll","No",1.3,26.4,134,27.7,3550,"40.25\"","34\"","34\"",290]
["YHJD60S43S3","208/230 3-60",23.9,40,"Scroll","No",1.5,17.899999999999999,120,19.399999999999999,3800,"40.25\"","34\"","34\"",280]
["YHJD60S43S4","208/230 3-60",22.9,40,"Scroll","No",1.3,17.3,115,18.600000000000001,3500,"40.25\"","34\"","34\"",280]
["YHJD60S43S5","208/230 3-60",21.2,35,"Scroll","No",1.3,15.9,110,17.2,3500,"40.25\"","34\"","34\"",280]
["YHJD60S44S3","460 3-60",12.8,20,"Scroll","No",0.8,9.6,70,10.4,3800,"40.25\"","34\"","34\"",280]
["YHJD60S44S4","460 3-60",12,20,"Scroll","No",0.8,9,53,9.8000000000000007,3800,"40.25\"","34\"","34\"",280]
["YHJD60S44S5","460 3-60",9.1,15,"Scroll","No",0.8,6.6,52,7.4,3500,"40.25\"","34\"","34\"",280]
["YHJF18S41S1","208/230 1-60",11.9,20,"Scroll","No",0.7,9,48,9.6999999999999993,2000,"28.25\"","34\"","34\"",145]
["YHJF24S41S1","208/230 1-60",17.600000000000001,30,"Scroll","No",0.8,13.4,58.3,14.200000000000001,2000,"40.25\"","29.5\"","29.5\"",145]
["YHJF30S41S1","208/230 1-60",17.3,30,"Scroll","No",1.3,12.8,64,14.100000000000001,3900,"40.25\"","34\"","34\"",176]
["YHJF36S41S1","208/230 1-60",23.7,40,"Scroll","No",1.3,17.899999999999999,96.7,19.2,3900,"40.25\"","34\"","34\"",193]
["YHJF36S41S4","208/230 1-60",19.7,30,"Recip","No",1.3,14.7,74,16,3800,"40.25\"","34\"","34\"",193]
["YHJF42S41S2","208/230 1-60",26.1,45,"Scroll","No",1.3,19.8,115,21.1,3900,"40.25\"","34\"","34\"",198]
["YHJF42S41S5","208/230 1-60",23.7,40,"Scroll","No",1.3,17.899999999999999,112,19.2,3600,"40.25\"","34\"","34\"",198]
["YHJF48S41S1","208/230 1-60",28.8,50,"Scroll","No",1.3,28.8,115,30.1,3800,"40.25\"","34\"","34\"",248]
["YHJF48S41S5","208/230 1-60",28.5,50,"Scroll","No",1.3,21.8,117,23.1,3500,"40.25\"","34\"","34\"",248]
["YHJF60S41S1","208/230 1-60",35.299999999999997,60,"Scroll","Yes",1.3,35.299999999999997,118,36.599999999999994,3800,"40.25\"","34\"","34\"",290]
["YHJF60T41S1","208/230 1-60",37.299999999999997,60,"Scroll","Yes",1.3,28.8,152.9,30.1,3450,"40.25\"","34\"","34\"",292]
["YZF02413C","208/230 1-60",17.5,30,"Scroll","No",0.7,13.4,58.3,14.1,2750,"40\"","37\"","31\"",199]
["YZF03013C","208/230 1-60",17.3,30,"Scroll","No",1.3,12.8,64,14.100000000000001,3800,"40\"","42.25\"","34\"",228]
["YZF03613C","208/230 1-60",22.6,35,"Scroll","No",1.3,17,77,18.3,3800,"40\"","42.25\"","34\"",230]
["YZF04214C","208/230 1-60",23.7,40,"Scroll","No",1.3,17.899999999999999,112,19.2,3800,"40\"","42.25\"","34\"",234]
["YZF04813C","208/230 1-60",26.9,45,"Scroll","No",1.3,20.5,115,21.8,3400,"40\"","42.25\"","34\"",283]
["YZF06013C","208/230 1-60",33.799999999999997,50,"Scroll","Yes",1.3,26,118,27.3,3700,"40\"","42.25\"","34\"",298]
["YZF06014C","208/230 1-60",33.799999999999997,60,"Scroll","Yes",1.3,28.8,152.9,30.1,3600,"40\"","42.25\"","34\"",298]
["YZH02411","208/230 1-60",18.2,30,"Scroll","Yes",2.8,12.3,52,15.100000000000001,2950,"40\"","42.25\"","34\"",315]
["YZH02412","208/230 1-60",17.5,25,"Scroll","Yes",2.8,11.8,58,14.600000000000001,2990,"40\"","42.25\"","34\"",295]
["YZH03611","208/230 1-60",23.6,40,"Scroll","Yes",2.8,16.600000000000001,82,19.400000000000002,3250,"40\"","42.25\"","34\"",315]
["YZH03612","208/230 1-60",21.8,35,"Scroll","Yes",2.8,15.2,83,18,3345,"40\"","42.25\"","34\"",295]
["YZH04811","208/230 1-60",29.2,50,"Scroll","Yes",2.8,21.1,96,23.900000000000002,3400,"40\"","42.25\"","34\"",320]
["YZH04812","208/230 1-60",29.2,50,"Scroll","Yes",2.8,21.1,104,23.900000000000002,3300,"40\"","42.25\"","34\"",320]
["YZH06011","208/230 1-60",34.799999999999997,60,"Scroll","Yes",2.8,25.6,118,28.400000000000002,3350,"40\"","42.25\"","34\"",340]
["YZH06012","208/230 1-60",36.9,60,"Scroll","Yes",2.8,27.3,153,30.1,3460,"40\"","42.25\"","34\"",325]
["THE30B31","208/230 3-60",12.42,20,"Scroll","No",1.3,9.9,58,11.200000000000001,2995,"39.5\"","35.25\"","31.75\"",176]
["THE36B31","208/230 3-60",12.58,20,"Recip","No",1.3,7.6,68,8.9,3715,"39.5\"","35.25\"","31.75\"",230]
["THE36B32","208/230 3-60",12.58,20,"Recip","No",1.3,7.6,68,8.9,3715,"39.5\"","35.25\"","31.75\"",230]
["THE42B31","208/230 3-60",16.100000000000001,25,"Recip","No",1.3,10.199999999999999,88,11.5,3715,"39.5\"","35.25\"","31.75\"",230]
["THE42B32","208/230 3-60",16.100000000000001,25,"Recip","No",1.3,10.199999999999999,88,11.5,3715,"39.5\"","35.25\"","31.75\"",230]
["THE42B33","208/230 3-60",16.100000000000001,25,"Recip","No",1.3,10.199999999999999,88,11.5,3715,"39.5\"","35.25\"","31.75\"",230]
["THE48B31","208/230 3-60",18.420000000000002,30,"Scroll","No",1.3,15.3,83.1,16.600000000000001,4100,"39.5\"","38.0\"","34.25\"",235]
["THE60B31","208/230 3-60",21.22,35,"Scroll","No",1.3,17.8,110,19.100000000000001,4100,"42.5\"","38.0\"","34.25\"",256]
["THE30B41","460 3-60",5.93,15,"Scroll","No",0.65,4.7,38,5.3500000000000005,2995,"39.5\"","35.25\"","31.75\"",176]
["THE36B41","460 3-60",7.05,15,"Recip","No",0.65,3.8,34,4.45,3715,"39.5\"","35.25\"","31.75\"",230]
["THE36B42","460 3-60",7.05,15,"Recip","No",0.65,3.8,34,4.45,3715,"39.5\"","35.25\"","31.75\"",230]
["THE42B41","460 3-60",7.25,15,"Recip","No",0.65,5.0999999999999996,44,5.75,3715,"39.5\"","35.25\"","31.75\"",230]
["THE42B42","460 3-60",7.25,15,"Recip","No",0.65,5.0999999999999996,44,5.75,3715,"39.5\"","35.25\"","31.75\"",230]
["THE42B43","460 3-60",7.25,15,"Recip","No",0.65,5.0999999999999996,44,5.75,3715,"39.5\"","35.25\"","31.75\"",230]
["THE48B41","460 3-60",8.66,15,"Scroll","No",0.6,6.9,41,7.5,4100,"39.5\"","38.0\"","34.25\"",235]
["THE60B41","460 3-60",10.33,15,"Scroll","No",0.6,8.6,52,9.1999999999999993,4100,"42.5\"","38.0\"","34.25\"",256]
["YHM24B21","208/230 1-60",17.2,30,"Rotary","No",1,13.19,"N/A",14.2,2850,33.25,"29.25\"","29.25\"",166]
["YHM36B21","208/230 1-60",21,35,"Rotary","No",1,15.2,"N/A",16.2,3715,"39.5\"","29.25\"","29.25\"",204]
["YHM36B22","208/230 1-60",21,35,"Rotary","No",1,15.2,"N/A",16.2,3715,"39.5\"","29.25\"","29.25\"",204]
["YHM48B21","208/230 1-60",35.6,60,"Rotary","No",1.3,27.42,"N/A",28.7,4000,"39.5\"","35.25\"","31.75\"",214]
["YHM60B21","208/230 1-60",34.700000000000003,60,"Rotary","No",1.3,23.73,"N/A",25,4100,"39.5\"","35.25\"","31.75\"",239]
["YZT24B21","208/230 1-60",15.3,25,"Scroll","Yes",2.8,10,62.9,12.8,2500,"39.5\"","35.25\"","31.75\"",176]
["YZT36B21","208/230 1-60",21.4,35,"Scroll","Yes",2.8,14.9,84.2,17.7,4000,"39.5\"","38.25\"","34.5\"",256]
["YZT48B21","208/230 1-60",28.2,45,"Scroll","Yes",2.8,20.399999999999999,122.1,23.2,4100,"46.5\"","38.25\"","34.5\"",292]
["YZT60B21","208/230 1-60",31.4,50,"Scroll","Yes",2.8,22.9,147.19999999999999,25.7,4100,"46.5\"","38.25\"","34.5\"",304]
["YHG18B21","208/230 1-60",14,20,"Scroll","No",2.8,9,47.5,11.8,2850,"36.25\"","29.5\"","29.5\"",136]
["YHG24B21","208/230 1-60",15.5,25,"Scroll","No",0.8,11.8,62.9,12.6,2995,"39.5\"","35.25\"","31.75\"",176]
["YHG30B21","208/230 1-60",19.600000000000001,30,"Scroll","No",2.8,13.4,72.5,16.2,2995,"39.5\"","35.25\"","31.75\"",176]
["YHG36B21","208/230 1-60",22,35,"Scroll","No",2.8,15.4,83.9,18.2,3715,"39.5\"","35.25\"","31.75\"",223]
["YHG42B21","208/230 1-60",28.7,45,"Scroll","No",2.8,20.7,123.9,23.5,3715,"39.5\"","38.0\"","31.75\"",270]
["YHG48B21","208/230 1-60",25.9,40,"Scroll","No",2.8,18.5,124,21.3,4100,"46.0\"","38.0\"","34.25\"",292]
["YHG60B21","208/230 1-60",32.4,50,"Scroll","No",2.8,23.68,152.5,26.5,4100,"46.0\"","38.0\"","34.25\"",304]
["YEE18B21","208/230 1-60",10.199999999999999,15,"Scroll","No",0.64,7.7,48,8.34,2000,"26.75\"","24.0\"","24\"",122]
["YEE24B21","208/230 1-60",14.1,20,"Scroll","No",0.64,10.8,55,11.440000000000001,2000,"33.25\"","24.0\"","24\"",131]
["YEE30B21","208/230 1-60",16.399999999999999,25,"Scroll","No",0.8,12.3,63,13.100000000000001,3200,"36.25\"","29.25\"","29.25\"",165]
["YEE36B21","208/230 1-60",19.600000000000001,30,"Scroll","No",1.3,14.7,75,16,4100,"36.25\"","35.25\"","31.75\"",191]
["YEE42B21","208/230 1-60",23.5,45,"Scroll","No",1.3,17.7,112.3,19,4100,"36.25\"","35.25\"","31.75\"",210]
["YEE48B21","208/230 1-60",24.5,45,"Scroll","No",1.3,18.5,108,19.8,4600,"39.5\"","38.0\"","34.25\"",224]
["YEE60B21","208/230 1-60",29.1,50,"Scroll","No",1.3,22.2,127.9,23.5,4800,"42.75\"","38.0\"","34.25\"",249]
["HMH72B241","208/230 1-60",15,25,"Twin Rotary","Yes","N/A",11,"N/A","N/A",880,"26.375\"","12.25\"","33.875\"",112]
["HMH72B361","208/230 1-60",23,35,"Twin Rotary","Yes","N/A",16.100000000000001,"N/A","N/A",810,"33.0\"","13.375\"","37.375\"",157]
["HMH72B481","208/230 1-60",36,50,"Twin Rotary","Yes","N/A",26,"N/A","N/A",850,"54.625\"","13.375\"","37.375\"",227]
["HMH72B601","208/230 1-60",37,50,"Twin Rotary","Yes","N/A",26.5,"N/A","N/A",850,"54.625\"","13.375\"","37.375\"",251]
["HMH72B341","208/230 1-60",23,35,"Twin Rotary","Yes","N/A",16.100000000000001,"N/A","N/A",810,"33.0\"","13.375\"","37.375\"",157]
["YH2E18SB21","208/230 1-60",9.1,15,"Scroll","No",0.64,6.8,41.7,7.4399999999999995,2100,"33.25\"","24.0\"","24.0\"",134]
["YH2E24TB21","208/230 1-60",13.4,20,"Scroll","Yes",0.64,10.199999999999999,55.2,10.84,2100,"36.25\"","24.0\"","24.0\"",140]
["YH2E30TB21","208/230 1-60",15.6,25,"Scroll","Yes",0.7,11.9,78,12.6,3000,"30.00\"","29.25\"","29.25\"",153]
["YH2E36TB21","208/230 1-60",20.3,35,"Scroll","Yes",1.3,15.2,78.099999999999994,16.5,3900,"33.25\"","35.25\"","31.75\"",183]
["YH2E42TB21","208/230 1-60",26.1,45,"Scroll","Yes",1.3,19.8,94,21.1,4100,"39.5\"","35.25\"","31.75\"",213]
["YH2E48TB21","208/230 1-60",26.1,45,"Scroll","Yes",1.3,19.8,109,21.1,4100,"39.5\"","35.25\"","31.75\"",215]
["YH2E60TB21","208/230 1-60",30.3,50,"Scroll","Yes",1.05,23.4,118,24.45,4700,"46.0\"","38.0\"","34.25\"",242]
["YH2F18SB21","208/230 1-60",9.1,15,"Scroll","No",0.64,6.8,41.7,7.4399999999999995,2100,"33.25\"","24.0\"","24.0\"",141]
["YH2F24TB21","208/230 1-60",14.2,25,"Scroll","Yes",0.64,10.9,61,11.540000000000001,2100,"36.25\"","24.0\"","24.0\"",147]
["YH2F30TB21","208/230 1-60",19,30,"Scroll","Yes",2.2000000000000002,13.4,87,15.600000000000001,2900,"36.25\"","29.25\"","29.25\"",177]
["YH2F36TB21","208/230 1-60",20.6,35,"Scroll","Yes",2.2000000000000002,14.7,102.1,16.899999999999999,3800,"39.5\"","35.25\"","31.75\"",204]
["YH2F42TB21","208/230 1-60",26.2,45,"Scroll","Yes",2.2000000000000002,19.2,123.5,21.4,4000,"39.5\"","35.25\"","31.75\"",232]
["YH2F48TB21","208/230 1-60",28.2,45,"Scroll","Yes",2.2000000000000002,20.8,142.5,23,3800,"39.5\"","38.0\"","34.25\"",243]
["YH2F60TB21","208/230 1-60",31.5,50,"Scroll","Yes",2.2000000000000002,23.4,118,25.599999999999998,4600,"39.5\"","38.0\"","34.25\"",282]
["YH418E2S11","208/230 1-60",9.1999999999999993,15,"Rotary","No",0.64,6.7,33,"N/A",2100,"36.25\"","24.0\"","24.0\"",124]
["YH424E2S11","208/230 1-60",13.5,20,"Scroll","Yes",0.7,10.199999999999999,62,"N/A",3000,"30.00\"","29.25\"","29.25\"",143]
["YH436E2S11","208/230 1-60",18.899999999999999,30,"Scroll","Yes",0.7,14.5,76,"N/A",3200,"36.25\"","29.25\"","29.25\"",165]
["YH448E2S11","208/230 1-60",26.3,45,"Scroll","Yes",1.3,20,141,"N/A",4100,"39.5\"","31.75\"","35.25\"",221]
["YH460E2S11","208/230 1-60",32.700000000000003,50,"Scroll","Yes",1.3,25.2,147.30000000000001,"N/A",3715,"39.5\"","31.75\"","35.25\"",239]
["HH824E2S11","208/230 1-60",24,35,"Rotary","Yes",0.8,16.8,"N/A","N/A",2235,"29.5\"","13.4\"","35.43\"",117]
["HH836E2S11","208/230 1-60",28,35,"Rotary","Yes",1.5,19,"N/A","N/A",3350,"34.45\"","17.72\"","43.33\"",185]
["HH860E2S11","208/230 1-60",37,45,"Rotary","Yes",1,27,"N/A","N/A",4820,"57/5\"","13.0\"","38.4\"",245]
["YH518E2S11","208/230 1-60",9.1999999999999993,15,"Rotary","No",0.64,6.7,33,"N/A",2100,"36.25\"","24.0\"","24.0\"",124]
["YH524E2S11","208/230 1-60",15,25,"Scroll","Yes",2.2000000000000002,10.199999999999999,62,"N/A",2900,"30.00\"","29.25\"","29.25\"",162]
["YH536E2S11","208/230 1-60",20.399999999999999,30,"Scroll","Yes",2.2000000000000002,14.5,76,"N/A",3055,"36.25\"","29.25\"","29.25\"",176]
["YH548E2S11","208/230 1-60",27.2,45,"Scroll","Yes",2.2000000000000002,20,141,"N/A",4000,"39.5\"","31.75\"","35.25\"",232]
["YH560E2S11","208/230 1-60",33.700000000000003,50,"Scroll","Yes",2.2000000000000002,25.2,147.30000000000001,"N/A",3975,"39.5\"","31.75\"","35.25\"",255]
["YH624E2S11","208/230 1-60",15,25,"Scroll","Yes",2.2000000000000002,10.199999999999999,62,"N/A",3055,"36.25\"","29.25\"","29.25\"",172]
["YH636E2S11","208/230 1-60",20.399999999999999,30,"Scroll","Yes",2.2000000000000002,14.5,76,"N/A",3755,"39.5\"","34.25\"","38\"",243]
["YH648E2S11","208/230 1-60",27.2,45,"Scroll","Yes",2.2000000000000002,20,141,"N/A",4200,"39.5\"","31.75\"","35.25\"",255]
["YH660E2S11","208/230 1-60",31.8,50,"Scroll","Yes",2.2000000000000002,23.7,123,"N/A",4760,"46\"","34.25\"","38\"",282]

{"sheet":"outdoor-images","index":6,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"IndoorUnitData","index":7,"n_rows":51,"n_cols":27,"rows_kept":51,"cut":false,"hidden":true,"merged":[]}
["Air Handler Style","AIR HANDLER MODEL","POWER SUPPLY","MIN CIRCUIT AMPACITY","MAX OVER-CURRENT PROTECTION","BLOWER TYPE","MOTOR F.L.A. @ 240 V","NOMINAL AIR FLOW (CFM)","MAX EXT. STATIC PRESSURE","HEIGHT","DEPTH","WIDTH","WEIGHT (lbs.)","Supply Duct Opening Depth (in)","Supply Duct Opening Width (in)","Return Duct Opening Depth (in)","Return Duct Opening Width (in)","Nominal","0.10","0.20","0.30","0.40","0.50","0.60","Factory Installed Metering Device","Air Filter Factory Installed","Air Filter Size (in)"]
["AM240","AM240AT","208/240 1-60",2,15,"3 Speed PSC",1.6,800,"0.50\"","36\"","22\"","15\"",80,"17\"","13\"","20.35\"","12.2\"",800,902,864,822,792,744,"N/A","TXV","NOT INCLUDED","12 X 20 X 1"]
["AM250","AM250AT","208/240 1-60",2.4,15,"3 Speed PSC",1.9,800,"0.50\"","41\"","22\"","18.5\"",105,"17\"","16.5\"","20.35\"","16.2\"",800,867,839,803,780,733,"N/A","TXV","NOT INCLUDED","16 X 20 X 1"]
["AM360","AM360BT","208/240 1-60",3.3,15,"3 Speed PSC",2.6,1200,"0.50\"","41\"","22\"","18.5\"",105,"17\"","16.5\"","20.35\"","16.2\"",1200,1268,1233,1186,1165,1133,"N/A","TXV","NOT INCLUDED","16 X 20 X 1"]
["AM370","AM370AT","208/240 1-60",2.4,15,"3 Speed PSC",1.9,1200,"0.50\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1200,1318,1299,1270,1210,1147,"N/A","TXV","NOT INCLUDED","18 X 25 X 1"]
["AM380","AM380CT","120 1-60",6.6,15,"3 Speed PSC",5.3,1200,"0.50\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1200,1190,1150,1100,1040,970,"N/A","TXV","NOT INCLUDED","18 X 25 X 1"]
["AM480","AM480CT","208/240 1-60",4.9000000000000004,15,"3 Speed PSC",3.9,1600,"0.50\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1600,1764,1709,1652,1563,1418,"N/A","TXV","NOT INCLUDED","18 X 25 X 1"]
["AM600","AM600CT","208/240 1-60",4.9000000000000004,15,"3 Speed PSC",3.9,2000,"0.50\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",2000,2031,1959,1832,1725,1617,"N/A","TXV","NOT INCLUDED","18 X 25 X 1"]
["AM601","AM601CT","120 1-60",13.1,15,"3 Speed PSC",10.5,2000,"0.50\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",2000,1972,1972,1968,1882,1819,"N/A","TXV","NOT INCLUDED","18 X 25 X 1"]
["AV240","AV240BT","208/240 1-60",3,15,"Variable Speed ECM",2.4,800,"0.80\"","48\"","22\"","18.5\"",130,"17\"","17\"","20\"","16\"",800,800,800,800,800,800,800,"TXV","INCLUDED","16 X 20 X 1"]
["AV300","AV300BT-120V","120 1-60",6.8,15,"Variable Speed ECM",4.8,1000,"0.80\"","48\"","22\"","18.5\"",130,"17\"","17\"","20\"","16\"",1000,1000,1000,1000,1000,1000,1000,"TXV","INCLUDED","16 X 20 X 1"]
["AV360","AV360CT","208/240 1-60",3.4,15,"Variable Speed ECM",2.7,1200,"0.80\"","49\"","26\"","20\"",150,"21\"","18.5\"","23.75\"","17.125\"",1200,1200,1200,1200,1200,1200,1200,"TXV","INCLUDED","16 X 24 X 1"]
["AV360","AV360CT-120V","120 1-60",6.8,15,"Variable Speed ECM",5.4,1200,"0.80\"","49\"","26\"","20\"",150,"21\"","18.5\"","23.75\"","17.125\"",1200,1200,1200,1200,1200,1200,1200,"TXV","INCLUDED","16 X 24 X 1"]
["AV480","AV480CT","208/240 1-60",4.4000000000000004,15,"Variable Speed ECM",3.5,1600,"0.80\"","49\"","26\"","20\"",230,"21\"","18.5\"","23.75\"","17.125\"",1600,1600,1600,1600,1600,1600,1600,"TXV","INCLUDED","16 X 24 X 1"]
["AV480","AV480CT-120V","120 1-60",8.8000000000000007,15,"Variable Speed ECM",7,1600,"0.80\"","49\"","26\"","20\"",230,"21\"","18.5\"","23.75\"","17.125\"",1600,1600,1600,1600,1600,1600,1600,"TXV","INCLUDED","16 X 24 X 1"]
["AV600","AV600CT","208/240 1-60",5.4,15,"Variable Speed ECM",4.3,1850,"0.80\"","53\"","26\"","22\"",240,"21\"","20.5\"","23.75\"","19.125\"",1850,1850,1850,1850,1850,1850,1850,"TXV","INCLUDED","18 X 24 X 1"]
["AV600","AV600CT-120V","120 1-60",10.8,15,"Variable Speed ECM",8.6,1850,"0.80\"","53\"","26\"","22\"",240,"21\"","20.5\"","23.75\"","19.125\"",1850,1850,1850,1850,1850,1850,1850,"TXV","INCLUDED","18 X 24 X 1"]
["AX182","AX182A*A+TXV","208/240 1-60",3.8,15,"5 Speed ECM",3,600,"0.60\"","36\"","22\"","15\"",80,"17\"","13\"","20.35\"","12.2\"",600,667,641,615,596,567,560,"TXV","NOT INCLUDED","12 X 20 X 1"]
["AX182","AX182ATA","208/240 1-60",3.8,15,"5 Speed ECM",3,600,"0.60\"","36\"","22\"","15\"",80,"17\"","13\"","20.35\"","12.2\"",600,667,641,615,596,567,560,"TXV","NOT INCLUDED","12 X 20 X 1"]
["AX240","AX240BN","208/240 1-60",3.8,15,"5 Speed ECM",3,800,"0.60\"","41\"","22\"","18.5\"",105,"17\"","16.5\"","20.35\"","16.2\"",800,892,859,832,818,790,775,"Piston","NOT INCLUDED","16 X 20 X 1"]
["AX240","AX240BT","208/240 1-60",3.8,15,"5 Speed ECM",3,800,"0.60\"","41\"","22\"","18.5\"",105,"17\"","16.5\"","20.35\"","16.2\"",800,892,859,832,818,790,775,"TXV","NOT INCLUDED","16 X 20 X 1"]
["AX241","AX241A*C+TXV","208/240 1-60",3.8,15,"5 Speed ECM",3,800,"0.60\"","36\"","22\"","15\"",80,"17\"","13\"","20.35\"","12.2\"",800,892,859,832,818,790,775,"TXV","NOT INCLUDED","12 X 20 X 1"]
["AX241","AX241B*C+TXV","208/240 1-60",3.8,15,"5 Speed ECM",3,800,"0.60\"","36\"","22\"","15\"",80,"17\"","13\"","20.35\"","12.2\"",800,892,859,832,818,790,775,"TXV","NOT INCLUDED","12 X 20 X 1"]
["AX241","AX241BT","208/240 1-60",3.8,15,"5 Speed ECM",3,800,"0.60\"","36\"","22\"","15\"",80,"17\"","13\"","20.35\"","12.2\"",800,892,859,832,818,790,775,"TXV","NOT INCLUDED","12 X 20 X 1"]
["AX242","AX242B*A+TXV","208/240 1-60",3.8,15,"5 Speed ECM",3,800,"0.60\"","41\"","22\"","18.5\"",105,"17\"","16.5\"","20.35\"","16.2\"",800,892,859,832,818,790,775,"TXV","NOT INCLUDED","16 X 20 X 1"]
["AX242","AX242BTA","208/240 1-60",3.8,15,"5 Speed ECM",3,800,"0.60\"","41\"","22\"","18.5\"",105,"17\"","16.5\"","20.35\"","16.2\"",800,892,859,832,818,790,775,"TXV","NOT INCLUDED","16 X 20 X 1"]
["AX300","AX300CN","208/240 1-60",3.8,15,"5 Speed ECM",3,1000,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1000,1085,1070,1048,1024,989,975,"Piston","NOT INCLUDED","18 X 25 X 1"]
["AX300","AX300CT","208/240 1-60",3.8,15,"5 Speed ECM",3,1000,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1000,1085,1070,1048,1024,989,975,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX310","AX310CT","208/240 1-60",3.8,15,"5 Speed ECM",3,1000,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1000,1085,1070,1048,1024,989,975,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX360","AX360C*A+TXV","208/240 1-60",3.8,15,"5 Speed ECM",3,1200,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1200,1270,1250,1238,1214,1179,1162,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX360","AX360CN","208/240 1-60",3.8,15,"5 Speed ECM",3,1200,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1200,1270,1250,1238,1214,1179,1162,"Piston","NOT INCLUDED","18 X 25 X 1"]
["AX360","AX360CT","208/240 1-60",3.8,15,"5 Speed ECM",3,1200,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1200,1270,1250,1238,1214,1179,1162,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX360","AX360CTA","208/240 1-60",3.8,15,"5 Speed ECM",3,1200,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1200,1270,1250,1238,1214,1179,1162,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX361","AX361C*C+TXV","208/240 1-60",3.8,15,"5 Speed ECM",3,1200,"0.60\"","41\"","22\"","18.5\"",105,"17\"","16.5\"","20.35\"","16.2\"",1200,1270,1250,1238,1214,1179,1162,"TXV","NOT INCLUDED","16 X 20 X 1"]
["AX361","AX361CT","208/240 1-60",3.8,15,"5 Speed ECM",3,1200,"0.60\"","41\"","22\"","18.5\"",105,"17\"","16.5\"","20.35\"","16.2\"",1200,1270,1250,1238,1214,1179,1162,"TXV","NOT INCLUDED","16 X 20 X 1"]
["AX362","AX362C*A+TXV","208/240 1-60",3.8,15,"5 Speed ECM",3,1200,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1200,1270,1250,1238,1214,1179,1162,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX362","AX362CTA","208/240 1-60",3.8,15,"5 Speed ECM",3,1200,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1200,1270,1250,1238,1214,1179,1162,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX420","AX420CT","208/240 1-60",3.8,15,"5 Speed ECM",3,1400,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1400,1447,1430,1404,1359,1322,1283,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX422","AX422CTA","208/240 1-60",3.8,15,"5 Speed ECM",3,1400,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1400,1447,1430,1404,1359,1322,1283,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX480","AX480C*A+TXV","208/240 1-60",4,15,"5 Speed ECM",3.2,1600,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1600,1675,1633,1579,1545,1487,1451,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX480","AX480C*C+TXV","208/240 1-60",4,15,"5 Speed ECM",3.2,1600,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1600,1675,1633,1579,1545,1487,1451,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX480","AX480CT","208/240 1-60",4,15,"5 Speed ECM",3.2,1600,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1600,1675,1633,1579,1545,1487,1451,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX481","AX481CT","208/240 1-60",4,15,"5 Speed ECM",3.2,1600,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1600,1675,1633,1579,1545,1487,1451,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX482","AX482C*A+TXV","208/240 1-60",5.8,15,"5 Speed ECM",4.5999999999999996,1600,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1600,1722,1666,1623,1564,1518,1471,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX482","AX482CTA","208/240 1-60",5.8,15,"5 Speed ECM",4.5999999999999996,1600,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",1600,1722,1666,1623,1564,1518,1471,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AV480","AV480C*+TXV","208/240 1-60",4.4000000000000004,15,"Variable Speed ECM",3.5,1600,"0.80\"","49\"","26\"","20\"",230,"21\"","18.5\"","23.75\"","17.125\"",1600,1600,1600,1600,1600,1600,1600,"TXV","INCLUDED","16 X 24 X 1"]
["AX600","AX600C*A+TXV","208/240 1-60",5.8,15,"5 Speed ECM",4.5999999999999996,2000,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",2000,2083,2048,2013,1972,1929,1885,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX600","AX600C*C+TXV","208/240 1-60",5.8,15,"5 Speed ECM",4.5999999999999996,2000,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",2000,2083,2048,2013,1972,1929,1885,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX600","AX600CT","208/240 1-60",5.8,15,"5 Speed ECM",4.5999999999999996,2000,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",2000,2083,2048,2013,1972,1929,1885,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX601","AX601CT","208/240 1-60",5.8,15,"5 Speed ECM",4.5999999999999996,2000,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",2000,2083,2048,2013,1972,1929,1885,"TXV","NOT INCLUDED","18 X 25 X 1"]
["AX602","AX602CT","208/240 1-60",5.8,15,"5 Speed ECM",4.5999999999999996,2000,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",2000,2083,2048,2013,1972,1929,1885,"TXV","NOT INCLUDED","18 X 25 X 1"]

{"sheet":"indoor-images","index":8,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"dimensions-images","index":9,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"Options","index":10,"n_rows":76,"n_cols":57,"rows_kept":76,"cut":false,"hidden":true,"merged":[]}
[]
[null,"Tonnage",null,"Outdoor Electric Service"]
[null,1.5,null,"Single Phase"]
[null,2,null,"3 Phase"]
[null,2.5]
[null,3]
[null,3.5]
[null,4]
[null,5]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["AHRI Reference Number","OEM Name","Outdoor Model","Indoor Model","Refrigerant","Capacity 95°F","EER","SEER","Airflow","Capacity 47°F","HSPF","Capacity 17°F","Metering Device Type","Metering device","Factory Installed","OUTDOOR MODEL2","POWER SUPPLY","MIN CIRCUIT AMPACITY","MAX OVER-CURRENT PROTECTION","COMPRESSOR TYPE","MULTI-STAGE COMPRESSOR","MOTOR R.L.A. @ 230 V","COMPRESSOR R.L.A. @ 230 v","COMPRESSOR L.R.A @ 230V","TOTAL F.L.A. @ 230 v","NOMINAL AIR FLOW (CFM)","HEIGHT","DEPTH","WIDTH","WEIGHT (lbs.)","Air Handler Style","AIR HANDLER MODEL","POWER SUPPLY2","MIN CIRCUIT AMPACITY3","MAX OVER-CURRENT PROTECTION4","BLOWER TYPE","MOTOR F.L.A. @ 240 V","NOMINAL AIR FLOW (CFM)5","MAX EXT. STATIC PRESSURE","HEIGHT6","DEPTH7","WIDTH8","WEIGHT (lbs.)9","Supply Duct Opening Depth (in)","Supply Duct Opening Width (in)","Return Duct Opening Depth (in)","Return Duct Opening Width (in)","Nominal","0.10","0.20","0.30","0.40","0.5","0.6","Factory Installed Metering Device","Air Filter Factory Installed","Air Filter Size (in)"]
[207768713,"YORK","HMH72B481","AX601CT","R-410A",48000,10,17,1500,45500,7.8,27800,"TXV","165616602A","Factory","HMH72B481","208/230 1-60",36,50,"Twin Rotary","Yes","N/A",26,"N/A","N/A",850,"54.625\"","13.375\"","37.375\"",227,"AX601","AX601CT","208/240 1-60",5.8,15,"5 Speed ECM",4.5999999999999996,2000,"0.60\"","48\"","26\"","21.875\"",155,"21\"","20\"","24.6\"","20.08\"",2000,2083,2048,2013,1972,1929,1885,"TXV","NOT INCLUDED","18 X 25 X 1"]

{"sheet":"Schedule","index":11,"n_rows":5,"n_cols":19,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[null," ","AHRI Number","OEM Name","Outside Model","Inside Model","Capacity2 95°F","SEER2","EER2","Airflow","Capacity2 47°F","HSPF2","Capacity2 17°F","Metering Device","Min Circuit Ampacity","Max Over-current Protection","Compressor Type","Multi-stage Compressor","Power Supply"]
[null,null,207768713,"YORK","HMH72B481","AX601CT",48000,17,10,1500,45500,7.8,27800,"165616602A",36,50,"Twin Rotary","Yes","208/230 1-60"]

{"sheet":"HP-Report","index":12,"n_rows":46,"n_cols":13,"rows_kept":46,"cut":false,"hidden":true,"merged":[[44,4,44,12],[45,4,45,12],[17,2,17,5],[24,2,24,5],[10,2,10,5],[35,4,35,9],[35,10,35,12],[27,2,27,4],[27,5,27,7],[29,2,29,7],[31,4,31,12],[16,2,16,7],[25,2,25,5],[26,2,26,7],[11,2,11,5],[12,2,12,5],[15,2,15,5],[14,2,14,5],[6,12,6,13],[5,1,5,2],[8,2,8,7],[5,3,5,4],[6,3,6,5],[6,7,6,9],[1,1,3,4],[1,6,1,10],[2,6,2,10],[3,5,3,13],[4,1,4,2],[4,10,4,11],[4,12,4,13],[4,3,4,9],[32,4,32,9],[32,10,32,12],[5,10,5,11],[5,12,5,13],[9,2,9,5],[9,9,28,12],[28,2,28,5],[18,2,18,5],[19,2,19,5],[20,2,20,7],[21,2,21,5],[22,2,22,5],[23,2,23,5],[13,2,13,5],[6,1,6,2],[6,10,6,11],[33,4,33,9],[33,10,33,12],[34,4,34,9],[34,10,34,12],[36,4,36,9],[40,4,40,12],[41,4,41,12],[42,4,42,12],[43,4,43,12],[37,10,37,12],[37,4,37,9]]}
[]
[null,null,null,null,null,null,"YORK"]
[null,null,null,null,null,null,"Split-System Heat Pump"]
[]
[null,"Project Name",null,null,null,null,null,null,null,null,"    Tag"]
[null,"Date",null,"2025-11-19",null,null,"     Quantity",null,null,null,"    Unit Model",null,"YORK HMH72B481"]
[null,"Engineer",null,null,null,null,"     Contractor",null,null,null,"    System",null,"HMH72B481, AX601CT"]
[]
[null,null,"Cooling & Matchup Performance"]
[null,null," AHRI Reference Number",null,null,null,207768713]
[null,null," Refrigerant Type",null,null,null,"R-410A"]
[null,null," Capacity",null,null,null,48000,"BTUH"]
[null,null," Energy Efficiency Ratio",null,null,null,10,"EER2"]
[null,null," Seasonal Energy Efficiency Ratio",null,null,null,17,"SEER2"]
[null,null," Airflow",null,null,null,1500,"CFM"]
[null,null," Metering Device Required",null,null,null,"TXV"]
[null,null,"Heat Pump Performance"]
[null,null," Heat Output (max) @47°F Ambient",null,null,null,45500,"BTUH"]
[null,null," Heat Output (max) @17°F Ambient",null,null,null,27800,"BTUH"]
[null,null," Heating Seasonal Performance Factor",null,null,null,7.8,"HSPF2"]
[null,null,"Physical & Electrical Data"]
[null,null," Power Supply",null,null,null,"208/230 1-60"]
[null,null," Unit Min Circuit Ampacity",null,null,null,36,"Amps"]
[null,null," Unit Max Over-Current Protection",null,null,null,50,"Amps"]
[null,null," Compressor Type",null,null,null,"Twin Rotary"]
[null,null," Multistage Compressor",null,null,null,"Yes"]
[null,null,"Dimensions & Weight"]
[null,null," Height x Length x Width",null,null,"54.625\" x 13.375\" x 37.375\""]
[null,null," Weight With Factory Installed Options",null,null,null,227,"lbs"]
[null,null,"Note : Please refer to the tech guide for any additional information"]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• 360 DC Inverter Driven Technology",null,null,null,null,null,"• Agency Listed"]
[null,null,null,null,"• Pressure Sensor",null,null,null,null,null,"• Side Discharge"]
[null,null,null,null,"• Small outdoor form factor for installation flexibility"]
[null,null,null,null,"   flexibility"]
[null,null,null,null,"• Stable temperature control means"]
[null,null,null,null,"   optimal comfort"]
[]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Extended 10-year limited parts warranty."]
[null,null,null,null,"• Extended 10-year limited compressor warranty"]
[null,null,null,null,"• Extended parts and compressor warranties require online registration within 90 days of"]
[null,null,null,null,"   purchase for replacement or closing for new home construction."]
[null,null,null,null,"   "]

{"sheet":"AC-Report","index":13,"n_rows":30,"n_cols":11,"rows_kept":30,"cut":false,"hidden":true,"merged":[[45,4,45,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[37,4,37,9],[37,10,37,12],[43,10,43,12],[44,4,44,9],[44,10,44,12],[40,10,40,12],[41,4,41,9],[41,10,41,12],[40,18,40,21],[28,2,28,5],[29,2,29,7],[33,18,33,21],[34,18,34,21],[35,18,35,21],[36,18,36,21],[37,18,37,21],[38,18,38,21],[39,18,39,21],[31,4,31,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[40,4,40,9],[47,18,47,21],[48,18,48,21],[41,18,41,21],[42,18,42,21],[43,18,43,21],[44,18,44,21],[46,18,46,21],[8,2,8,7],[9,2,9,5],[9,9,28,12],[10,2,10,5],[11,2,11,5],[12,2,12,5],[13,2,13,5],[15,2,15,5],[16,2,20,7],[21,2,21,5],[22,2,22,5],[23,2,23,5],[24,2,24,5],[25,2,25,5],[26,2,26,7],[27,2,27,4],[5,1,5,2],[5,3,5,7],[5,10,5,11],[5,12,5,13],[6,1,6,2],[6,10,6,11],[6,12,6,13],[1,1,3,4],[1,6,1,10],[2,6,2,10],[3,5,3,13],[4,1,4,2],[4,3,4,4],[4,10,4,11],[4,12,4,13],[14,2,14,5],[50,4,50,12],[46,4,46,12],[47,4,47,12],[48,4,48,12],[49,4,49,12],[42,4,42,9],[42,10,42,12],[43,4,43,9],[27,5,27,7],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[34,4,34,9],[34,10,34,12]]}
[]
[]
[null,null,null,null,null,null,"Air Conditioners"]
[]
[null,"Date",null,null,null,null,null,null,null,null,"Tag"]
[null,"Project Name",null,null,null,null,null,null,null,null,"Unit Model"]
[null,"Quantity",null,null,null,null,null,null,null,null,"System"]
[]
[null,null,"Cooling & Matchup Performance"]
[null,null,"AHRI Reference Number"]
[null,null,"Refrigerant Type"]
[null,null,"Capacity",null,null,null,null,"BTUH"]
[null,null,"Energy Efficiency Ratio",null,null,null,null,"EER"]
[null,null,"Seasonal Energy Efficiency Ratio",null,null,null,null,"SEER"]
[null,null,"Airflow",null,null,null,null,"CFM"]
[null,null,"Metering Device Required"]
[null,null,"Physical & Electrical Data"]
[]
[]
[]
[]
[null,null,"Power Supply"]
[null,null,"Unit Min Circuit Ampacity",null,null,null,null,"Amps"]
[null,null,"Unit Max Over-Current Protection",null,null,null,null,"Amps"]
[null,null,"Compressor Type"]
[null,null,"Multistage Compressor"]
[null,null,"Dimensions & Weight"]
[null,null,"Height x Length x Width (inches)"]
[null,null,"Weight With Factory Installed Options",null,null,null,null,"lbs"]
[null,null,"Note : Please refer to the tech guide for listed maximum static pressures"]

{"sheet":"Indoor-Report","index":14,"n_rows":51,"n_cols":13,"rows_kept":51,"cut":false,"hidden":true,"merged":[[14,2,14,5],[5,1,5,2],[8,2,8,7],[9,2,9,5],[9,9,33,12],[10,2,10,5],[11,2,11,5],[12,2,12,5],[13,2,13,5],[15,2,15,5],[16,2,16,7],[17,2,17,5],[5,10,5,11],[5,12,5,13],[6,1,6,2],[6,10,6,11],[6,12,6,13],[6,7,6,9],[6,3,6,5],[5,3,5,4],[1,1,3,4],[1,6,1,10],[3,5,3,13],[4,1,4,2],[4,10,4,11],[4,12,4,13],[2,6,2,10],[4,3,4,9],[28,2,28,5],[17,6,17,7],[18,2,18,5],[19,2,19,5],[20,2,20,5],[21,2,21,5],[22,2,22,5],[23,2,23,5],[24,2,24,5],[25,2,25,5],[26,2,26,7],[27,2,27,5],[29,2,29,5],[30,2,30,5],[31,2,31,7],[32,2,32,4],[32,5,32,7],[33,2,33,5],[34,2,34,7],[36,4,36,12],[37,4,37,12],[38,4,38,12],[48,4,48,12],[49,4,49,12],[50,4,50,12],[51,4,51,12],[39,4,39,12],[40,4,40,12],[41,4,41,12],[44,4,44,12],[42,4,42,12],[43,4,43,12],[47,4,47,12],[46,4,46,12],[45,4,45,12]]}
[]
[null,null,null,null,null,null,"ADP"]
[null,null,null,null,null,null,"Indoor Air Handler"]
[]
[null,"Project Name",null,null,null,null,null,null,null,null,"    Tag"]
[null,"Date",null,"2025-11-19",null,null,"     Quantity",null,null,null,"    Unit Model",null,"AX601CT"]
[null,"Engineer",null,null,null,null,"     Contractor",null,null,null,"    System",null,"(YORK) HMH72B481, AX601CT"]
[]
[null,null,"Cooling & Matchup Performance"]
[null,null," AHRI Reference Number",null,null,null,207768713]
[null,null," Refrigerant Type",null,null,null,"R-410A"]
[null,null," Capacity",null,null,null,48000,"BTUH"]
[null,null," Energy Efficiency Ratio",null,null,null,10,"EER2"]
[null,null," Seasonal Energy Efficiency Ratio",null,null,null,17,"SEER2"]
[null,null," Airflow",null,null,null,1500,"CFM"]
[null,null," Metering Device Required",null,null,null,"TXV"]
[null,null,"Supply Air Blower*"]
[null,null," Blower Type",null,null,null,"5 Speed ECM"]
[null,null," Airflow",null,null,null,2000,"CFM"]
[null,null," Max External Static Pressure",null,null,null,"0.60\"","W.C."]
[null,null," Flow @ 0.10\" W.C.",null,null,null,2083,"CFM"]
[null,null," Flow @ 0.20\" W.C.",null,null,null,2048,"CFM"]
[null,null," Flow @ 0.30\" W.C.",null,null,null,2013,"CFM"]
[null,null," Flow @ 0.40\" W.C.",null,null,null,1972,"CFM"]
[null,null," Flow @ 0.50\" W.C.",null,null,null,1929,"CFM"]
[null,null," Flow @ 0.60\" W.C.",null,null,null,1885,"CFM"]
[null,null,"Physical & Electrical Data†"]
[null,null," Power Supply",null,null,null,"208/240 1-60"]
[null,null," Unit Min Circuit Ampacity",null,null,null,5.8,"Amps"]
[null,null," Unit Max Over-Current Protection",null,null,null,15,"Amps"]
[null,null,{"$f":"\" \"&VLOOKUP('Indoor-Report'!G10,HPRatings!$A$2:$P$306,15,FALSE)&\" installed Metering Device\"","v":" Factory installed Metering Device"},null,null,null,"TXV"]
[null,null,"Dimensions & Weight"]
[null,null," Height x Depth x Width",null,null,"48\" x 26\" x 21.875\""]
[null,null," Weight With Factory Installed Options",null,null,null,155,"lbs"]
[null,null,"*Data shown is for factory motor speed setting.\n†Electrical data does not include field installed heat."]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Cabinet constructed of heavy gauge painted steel for additional corrosion resistance."]
[null,null,null,null,"• High quality 5/8\" foil-faced insulation lines cabinet, with cabinet flanges & retaining rods for"]
[null,null,null,null,"better attachment."]
[null,null,null,null,"• Independent lab tested 2% or less air leakage for better efficiency."]
[null,null,null,null,"• Coils are air pressure tested at 500 PSI, leak tested with helium, sealed with rubber plugs, then "]
[null,null,null,null,"charged with dry air."]
[null,null,null,null,"• HYDROTECTM drain pans hold less water, which reduces the possibility of mold and mildew"]
[null,null,null,null,"growing in the pan. "]
[null,null,null,null,"• All drain pans have Microban protection, which inhibits the growth of mold and mildew that"]
[null,null,null,null,"cause odors and staining. "]
[null,null,null,null,"• Fan time delay factory installed (1 second on, 45 seconds off)."]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• AX Series air handlers feature a standard 5-year limited warranty; a 10-year limited warranty is ",null,null,null,null,"Low Maintenance"]
[null,null,null,null,"available with registration."]

{"sheet":"AM-Dimension","index":15,"n_rows":39,"n_cols":13,"rows_kept":39,"cut":false,"hidden":true,"merged":[[38,2,39,12],[37,2,37,12],[14,4,14,12],[5,1,5,2],[6,1,6,2],[9,4,9,12],[10,4,10,12],[11,4,11,12],[12,4,12,12],[13,4,13,12],[5,12,5,13],[6,12,6,13],[5,10,5,11],[6,10,6,11],[35,9,35,11],[35,2,35,3],[1,1,3,4],[1,6,1,10],[2,6,2,10],[3,5,3,13],[4,1,4,2],[4,12,4,13],[4,10,4,11],[4,3,4,9],[5,3,5,4],[6,3,6,5],[6,7,6,9],[35,7,35,8],[15,9,15,12],[34,7,34,8],[32,2,32,12],[33,7,33,11],[34,9,34,11],[33,4,33,6],[33,2,34,3]]}
[]
[null,null,null,null,null,null,"ADP"]
[null,null,null,null,null,null,"Indoor Air Handler"]
[]
[null,"Project Name",null,null,null,null,null,null,null,null,"    Tag"]
[null,"Date",null,null,null,null,"     Quantity",null,null,null,"    Unit Model"]
[null,"Engineer",null,null,null,null,"     Contractor","",null,null,"    System"]
[]
[]
[null,null,null,null,null,null,null,null,null,"Secured  Service  Valves"]
[null,null,null,null,null,null,null,null,null,"Agency Listed"]
[null,null,null,null,null,null,null,null,null,"Warranty *"]
[null,null,null,null,null,null,null,null,null,"Standard 5-Years limited parts warranty."]
[null,null,null,null,null,null,null,null,null,"Standard 10-Years limited compressor warranty."]
[null,null,null,null,null,null,null,null,null,"Extended 10-Years limited parts warranty when product is registered online within 90 days of purchase for replacement or closing for new home construction."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Air Handler Size"]
[null,null,"Model",null,"Overall Dimensions",null,null,"Supply Duct Opening",null,null,null,null,"Return Duct Opening"]
[null,null,null,null,"A","B"," C","Depth",null,"Width",null,null,"Depth               Width"]
[]
[]
[null,null,"Clearance Information"]
[null,null,"Clearance to combustible material to be 0 inches to unit casing, and 0 inches to plenum and duct for the first 36 inches."]

{"sheet":"AV-Dimension","index":16,"n_rows":39,"n_cols":13,"rows_kept":39,"cut":false,"hidden":true,"merged":[[37,2,37,12],[38,2,39,12],[1,1,3,4],[1,6,1,10],[2,6,2,10],[3,5,3,13],[4,1,4,2],[4,10,4,11],[4,12,4,13],[14,4,14,12],[5,1,5,2],[6,1,6,2],[9,4,9,12],[10,4,10,12],[13,4,13,12],[5,10,5,11],[5,12,5,13],[6,10,6,11],[6,12,6,13],[4,3,4,9],[5,3,5,4],[6,3,6,5],[6,7,6,9],[11,4,11,12],[12,4,12,12],[35,2,35,3],[35,7,35,8],[15,9,15,12],[34,7,34,8],[32,2,32,12],[33,7,33,11],[34,9,34,11],[35,9,35,11],[33,2,34,3],[33,4,33,6]]}
[]
[null,null,null,null,null,null,"ADP"]
[null,null,null,null,null,null,"Indoor Air Handler"]
[]
[null,"Project Name",null,null,null,null,null,null,null,null,"    Tag"]
[null,"Date",null,null,null,null,"     Quantity",null,null,null,"    Unit Model"]
[null,"Engineer",null,null,null,null,"     Contractor","",null,null,"    System"]
[]
[]
[null,null,null,null,null,null,null,null,null,"Secured  Service  Valves"]
[null,null,null,null,null,null,null,null,null,"Agency Listed"]
[null,null,null,null,null,null,null,null,null,"Warranty *"]
[null,null,null,null,null,null,null,null,null,"Standard 5-Years limited parts warranty."]
[null,null,null,null,null,null,null,null,null,"Standard 10-Years limited compressor warranty."]
[null,null,null,null,null,null,null,null,null,"Extended 10-Years limited parts warranty when product is registered online within 90 days of purchase for replacement or closing for new home construction."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Air Handler Size"]
[null,null,"Model",null,"Overall Dimensions",null,null,"Supply Duct Opening",null,null,null,null,"Return Duct Opening"]
[null,null,null,null,"A","B"," C","Depth",null,"Width",null,null,"Depth               Width"]
[]
[]
[null,null,"Clearance Information"]
[null,null,"Clearance to combustible material to be 0 inches to unit casing, and 0 inches to plenum and duct for the first 36 inches."]

{"sheet":"AX-Dimension","index":17,"n_rows":39,"n_cols":13,"rows_kept":39,"cut":false,"hidden":true,"merged":[[37,2,37,12],[38,2,39,12],[32,2,32,12],[33,7,33,11],[5,1,5,2],[6,1,6,2],[9,4,9,12],[10,4,10,12],[11,4,11,12],[12,4,12,12],[13,4,13,12],[14,4,14,12],[15,9,15,12],[5,10,5,11],[5,12,5,13],[6,10,6,11],[35,2,35,3],[35,7,35,8],[34,7,34,8],[34,9,34,11],[35,9,35,11],[33,2,34,3],[33,4,33,6],[5,3,5,4],[6,3,6,5],[6,7,6,9],[1,1,3,4],[1,6,1,10],[3,5,3,13],[4,1,4,2],[2,6,2,10],[4,10,4,11],[4,12,4,13],[4,3,4,9],[6,12,6,13]]}
[]
[null,null,null,null,null,null,"ADP"]
[null,null,null,null,null,null,"Indoor Air Handler"]
[]
[null,"Project Name",null,null,null,null,null,null,null,null,"    Tag"]
[null,"Date",null,"2025-11-19",null,null,"     Quantity",null,null,null,"    Unit Model",null,"AX601CT"]
[null,"Engineer",null,null,null,null,"     Contractor",null,null,null,"    System",null,"HMH72B481, AX601CT"]
[]
[]
[null,null,null,null,null,null,null,null,null,"Secured  Service  Valves"]
[null,null,null,null,null,null,null,null,null,"Agency Listed"]
[null,null,null,null,null,null,null,null,null,"Warranty *"]
[null,null,null,null,null,null,null,null,null,"Standard 5-Years limited parts warranty."]
[null,null,null,null,null,null,null,null,null,"Standard 10-Years limited compressor warranty."]
[null,null,null,null,null,null,null,null,null,"Extended 10-Years limited parts warranty when product is registered online within 90 days of purchase for replacement or closing for new home construction."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"18 X 25 X 1 FILTER NOT INCLUDED"]
[]
[null,null,"Air Handler Size"]
[null,null,"Model",null,"Overall Dimensions",null,null,"Supply Duct Opening",null,null,null,null,"Return Duct Opening"]
[null,null,null,null,"A","B"," C","Depth",null,"Width",null,null,"Depth               Width"]
[null,null,"AX601",null,"48\"","26\"","21.875\"","21\"",null,"20\"",null,null,"24.6\"               20.08\""]
[]
[null,null,"Clearance Information"]
[null,null,"Clearance to combustible material to be 0 inches to unit casing, and 0 inches to plenum and duct for the first 36 inches."]

{"sheet":"THGD_YORK_SUMMARY","index":18,"n_rows":45,"n_cols":11,"rows_kept":45,"cut":false,"hidden":true,"merged":[[35,4,35,9],[35,10,35,12],[40,4,40,12],[41,4,41,12],[42,4,42,12],[31,4,31,12],[34,4,34,9],[34,10,34,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[45,4,45,12],[36,4,36,9],[36,10,36,12],[37,4,37,9],[37,10,37,12],[43,4,43,12],[44,4,44,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Small Footprint",null,null,null,null,null,"• Top Discharge"]
[null,null,null,null,"• Quality Condenser Coils ",null,null,null,null,null,"• Low Operating Sound Level"]
[null,null,null,null,"• Coil Protection ",null,null,null,null,null,"• Low Maintenance"]
[null,null,null,null,"• Protected Compressor",null,null,null,null,null,"• Easy Service Access"]
[null,null,null,null,"• Environmentally Friendly Refrigerant",null,null,null,null,null,"• Secured Service Valves"]
[null,null,null,null,"• Durable Finish",null,null,null,null,null,"• Agency Listed"]
[null,null,null,null,"• Lower Installed Cost"]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Standard 5-Years limited parts warranty."]
[null,null,null,null,"• Standard 5-Years limited compressor warranty."]
[null,null,null,null,"• Extended 10-Years limited parts and compressor warranty when product is registered "]
[null,null,null,null,"   online within 90 days of purchase for replacement or closing for new home construction."]

{"sheet":"YHJD_YORK_SUMMARY","index":19,"n_rows":46,"n_cols":11,"rows_kept":46,"cut":false,"hidden":true,"merged":[[34,4,34,9],[34,10,34,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[40,4,40,12],[37,4,37,9],[37,10,37,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[42,4,42,12],[43,4,43,12],[44,4,44,12],[45,4,45,12],[41,4,41,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Small Footprint",null,null,null,null,null,"• Top Discharge"]
[null,null,null,null,"• Quality Condenser Coils ",null,null,null,null,null,"• Low Operating Sound Level"]
[null,null,null,null,"• Coil Protection ",null,null,null,null,null,"• Low Maintenance"]
[null,null,null,null,"• Protected Compressor",null,null,null,null,null,"• Easy Service Access"]
[null,null,null,null,"• Environmentally Friendly Refrigerant",null,null,null,null,null,"• Secured Service Valves"]
[null,null,null,null,"• Durable Finish",null,null,null,null,null,"• Agency Listed"]
[null,null,null,null,"• Lower Installed Cost"]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Standard 5-Years limited parts warranty (1-Year on 3 phase models)."]
[null,null,null,null,"• Standard 10-Years limited compressor warranty (5-Years on 3 phase models)."]
[null,null,null,null,"• Extended 10-Years limited parts warranty when product is registered online within 90"]
[null,null,null,null,"   days of purchase for replacement or closing for new home construction (not available"]
[null,null,null,null,"   on 3 phase models)."]

{"sheet":"YHM_YORK_SUMMARY","index":20,"n_rows":46,"n_cols":11,"rows_kept":46,"cut":false,"hidden":true,"merged":[[42,4,42,12],[43,4,43,12],[44,4,44,12],[45,4,45,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[40,4,40,12],[41,4,41,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[37,4,37,9],[37,10,37,12],[34,4,34,9],[34,10,34,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Easier Installation",null,null,null,null,null,"• Environmentally Friendly"]
[null,null,null,null,"• Accessible Information",null,null,null,null,null,"• Top Discharge"]
[null,null,null,null,"• Durable Finish",null,null,null,null,null,"• Low Operating Sound Levels"]
[null,null,null,null,"• Rugged Coil Protection",null,null,null,null,null,"• Better Service Access"]
[null,null,null,null,"• Quality Coils",null,null,null,null,null,"• Agency Listed"]
[null,null,null,null,"• Protected Compressor",null,null,null,null,null,"• Improved Temperature Control"]
[null,null,null,null,"• Reliable Operation"]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Standard 5-Years limited parts warranty."]
[null,null,null,null,"• Standard 10-Years limited compressor warranty."]
[null,null,null,null,"• Extended 10-Years limited parts warranty when product is registered online within 90"]
[null,null,null,null,"   days of purchase for replacement or closing for new home construction."]
[null,null,null,null,"   "]

{"sheet":"HMH_YORK_SUMMARY","index":21,"n_rows":46,"n_cols":11,"rows_kept":46,"cut":false,"hidden":true,"merged":[[42,4,42,12],[43,4,43,12],[44,4,44,12],[45,4,45,12],[35,4,35,9],[40,4,40,12],[41,4,41,12],[37,4,37,9],[35,10,35,12],[36,4,36,9],[37,10,37,12],[34,4,34,9],[34,10,34,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• 360 DC Inverter Driven Technology",null,null,null,null,null,"• Agency Listed"]
[null,null,null,null,"• Pressure Sensor",null,null,null,null,null,"• Side Discharge"]
[null,null,null,null,"• Small outdoor form factor for installation flexibility"]
[null,null,null,null,"   flexibility"]
[null,null,null,null,"• Stable temperature control means"]
[null,null,null,null,"   optimal comfort"]
[]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Extended 10-year limited parts warranty."]
[null,null,null,null,"• Extended 10-year limited compressor warranty"]
[null,null,null,null,"• Extended parts and compressor warranties require online registration within 90 days of"]
[null,null,null,null,"   purchase for replacement or closing for new home construction."]
[null,null,null,null,"   "]

{"sheet":"THE_YORK_SUMMARY","index":22,"n_rows":44,"n_cols":11,"rows_kept":44,"cut":false,"hidden":true,"merged":[[34,4,34,9],[34,10,34,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[37,4,37,9],[37,10,37,12],[42,4,42,12],[43,4,43,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[40,4,40,12],[41,4,41,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Easier Installation",null,null,null,null,null,"• Environmentally Friendly"]
[null,null,null,null,"• Accessible Information",null,null,null,null,null,"• Top Discharge"]
[null,null,null,null,"• Durable Finish",null,null,null,null,null,"• Low Operating Sound Levels"]
[null,null,null,null,"• Rugged Coil Protection",null,null,null,null,null,"• Better Service Access"]
[null,null,null,null,"• Quality Coils",null,null,null,null,null,"• Agency Listed"]
[null,null,null,null,"• Protected Compressor"]
[null,null,null,null,"• Reliable Operation"]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Standard 1-Year limited parts warranty."]
[null,null,null,null,"• Standard 5-Years limited compressor warranty."]
[null,null,null,null,"   "]

{"sheet":"YHE_YORK_SUMMARY","index":23,"n_rows":46,"n_cols":11,"rows_kept":46,"cut":false,"hidden":true,"merged":[[42,4,42,12],[43,4,43,12],[44,4,44,12],[45,4,45,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[40,4,40,12],[41,4,41,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[37,4,37,9],[37,10,37,12],[34,4,34,9],[34,10,34,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Easier Installation",null,null,null,null,null,"• Environmentally Friendly"]
[null,null,null,null,"• Accessible Information",null,null,null,null,null,"• Top Discharge"]
[null,null,null,null,"• Durable Finish",null,null,null,null,null,"• Low Operating Sound Levels"]
[null,null,null,null,"• Rugged Coil Protection",null,null,null,null,null,"• Better Service Access"]
[null,null,null,null,"• Quality Coils",null,null,null,null,null,"• Agency Listed"]
[null,null,null,null,"• Protected Compressor"]
[null,null,null,null,"• Reliable Operation"]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Standard 5-Years limited parts warranty."]
[null,null,null,null,"• Standard 10-Years limited compressor warranty."]
[null,null,null,null,"• Extended 10-Years limited parts warranty when product is registered online within 90"]
[null,null,null,null,"   days of purchase for replacement or closing for new home construction."]
[null,null,null,null,"   "]

{"sheet":"YH2E_YORK_SUMMARY","index":24,"n_rows":46,"n_cols":11,"rows_kept":46,"cut":false,"hidden":true,"merged":[[34,4,34,9],[34,10,34,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[37,4,37,9],[37,10,37,12],[42,4,42,12],[43,4,43,12],[44,4,44,12],[45,4,45,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[40,4,40,12],[41,4,41,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Easier Installation",null,null,null,null,null,"• Environmentally Friendly"]
[null,null,null,null,"• Accessible Information",null,null,null,null,null,"• Top Discharge"]
[null,null,null,null,"• Durable Finish",null,null,null,null,null,"• Low Operating Sound Levels"]
[null,null,null,null,"• Rugged Coil Protection",null,null,null,null,null,"• Better Service Access"]
[null,null,null,null,"• Quality Coils",null,null,null,null,null,"• Agency Listed"]
[null,null,null,null,"• Protected Compressor"]
[null,null,null,null,"• Reliable Operation"]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Standard 5-Years limited parts warranty."]
[null,null,null,null,"• Standard 10-Years limited compressor warranty."]
[null,null,null,null,"• Extended 10-Years limited parts warranty when product is registered online within 90"]
[null,null,null,null,"   days of purchase for replacement or closing for new home construction."]
[null,null,null,null,"   "]

{"sheet":"YH2F_YORK_SUMMARY","index":25,"n_rows":46,"n_cols":11,"rows_kept":46,"cut":false,"hidden":true,"merged":[[34,4,34,9],[34,10,34,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[37,4,37,9],[37,10,37,12],[42,4,42,12],[43,4,43,12],[44,4,44,12],[45,4,45,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[40,4,40,12],[41,4,41,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Easier Installation",null,null,null,null,null,"• Environmentally Friendly"]
[null,null,null,null,"• Accessible Information",null,null,null,null,null,"• Top Discharge"]
[null,null,null,null,"• Durable Finish",null,null,null,null,null,"• Low Operating Sound Levels"]
[null,null,null,null,"• Rugged Coil Protection",null,null,null,null,null,"• Better Service Access"]
[null,null,null,null,"• Quality Coils",null,null,null,null,null,"• Agency Listed"]
[null,null,null,null,"• Protected Compressor"]
[null,null,null,null,"• Reliable Operation"]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Standard 5-Years limited parts warranty."]
[null,null,null,null,"• Standard 10-Years limited compressor warranty."]
[null,null,null,null,"• Extended 10-Years limited parts warranty when product is registered online within 90"]
[null,null,null,null,"   days of purchase for replacement or closing for new home construction."]
[null,null,null,null,"   "]

{"sheet":"YEE_YORK_SUMMARY","index":26,"n_rows":46,"n_cols":11,"rows_kept":46,"cut":false,"hidden":true,"merged":[[34,4,34,9],[34,10,34,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[37,4,37,9],[37,10,37,12],[42,4,42,12],[43,4,43,12],[44,4,44,12],[45,4,45,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[40,4,40,12],[41,4,41,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Easier Installation",null,null,null,null,null,"• Environmentally Friendly"]
[null,null,null,null,"• Accessible Information",null,null,null,null,null,"• Top Discharge"]
[null,null,null,null,"• Durable Finish",null,null,null,null,null,"• Low Operating Sound Levels"]
[null,null,null,null,"• Rugged Coil Protection",null,null,null,null,null,"• Better Service Access"]
[null,null,null,null,"• Quality Coils",null,null,null,null,null,"• Agency Listed"]
[null,null,null,null,"• Protected Compressor"]
[null,null,null,null,"• Reliable Operation"]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Standard 5-Years limited parts warranty."]
[null,null,null,null,"• Standard 10-Years limited compressor warranty."]
[null,null,null,null,"• Extended 10-Years limited parts warranty when product is registered online within 90"]
[null,null,null,null,"   days of purchase for replacement or closing for new home construction."]
[null,null,null,null,"   "]

{"sheet":"YHG_YORK_SUMMARY","index":27,"n_rows":46,"n_cols":11,"rows_kept":46,"cut":false,"hidden":true,"merged":[[34,4,34,9],[34,10,34,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[37,4,37,9],[37,10,37,12],[42,4,42,12],[43,4,43,12],[44,4,44,12],[45,4,45,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[40,4,40,12],[41,4,41,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Easier Installation",null,null,null,null,null,"• Top Discharge"]
[null,null,null,null,"• Accessible Information",null,null,null,null,null,"• Low Operating Sound Levels"]
[null,null,null,null,"• Durable Finish",null,null,null,null,null,"• Better Service Access"]
[null,null,null,null,"• Rugged Coil Protection",null,null,null,null,null,"• Agency Listed"]
[null,null,null,null,"• Protected Compressor"]
[null,null,null,null,"• Reliable Operation"]
[null,null,null,null,"• Environmentally Friendly"]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Extended 10-Years limited parts warranty."]
[null,null,null,null,"• Standard 10-Years limited compressor warranty."]
[null,null,null,null,"• Extended 10-Years limited parts warranty requires online registration within 90"]
[null,null,null,null,"   days of purchase for replacement or closing for new home construction."]
[null,null,null,null,"   "]

{"sheet":"YZT_YORK_SUMMARY","index":28,"n_rows":46,"n_cols":11,"rows_kept":46,"cut":false,"hidden":true,"merged":[[34,4,34,9],[34,10,34,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[37,4,37,9],[37,10,37,12],[42,4,42,12],[43,4,43,12],[44,4,44,12],[45,4,45,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[40,4,40,12],[41,4,41,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Superior Coil Protection",null,null,null,null,null,"• High-Efficiency Outdoor Coil"]
[null,null,null,null,"• Environmentally Friendly",null,null,null,null,null,"• Factory Installed Filter Drier"]
[null,null,null,null,"• Durable Finish",null,null,null,null,null,"• Climate SetTM"]
[null,null,null,null,"• QuitDriveTM System",null,null,null,null,null,"• Better Service Access"]
[null,null,null,null,"• ECM Fan Motor",null,null,null,null,null,"• Easy Service Access"]
[null,null,null,null,"• Swept Wing Fan",null,null,null,null,null,"• TXV Controls"]
[null,null,null,null,"• Composite Base Pan",null,null,null,null,null,"• Communications Capable"]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Extended 10-Years limited parts warranty"]
[null,null,null,null,"• Extended Lifetime limited compressor warranty."]
[null,null,null,null,"• Extended parts and compressor warranties require online registration within 90 days"]
[null,null,null,null,"   of purchase for replacement or closing for new home construction."]
[null,null,null,null,"   "]

{"sheet":"YHJF_YORK_SUMMARY","index":29,"n_rows":45,"n_cols":11,"rows_kept":45,"cut":false,"hidden":true,"merged":[[44,4,44,12],[37,4,37,9],[37,10,37,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[34,4,34,9],[34,10,34,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[38,4,38,9],[38,10,38,12],[40,4,40,12],[41,4,41,12],[42,4,42,12],[43,4,43,12],[39,4,39,9],[39,10,39,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Small Footprint",null,null,null,null,null,"• Top Discharge"]
[null,null,null,null,"• Quality Condenser Coils ",null,null,null,null,null,"• Quiet Operation"]
[null,null,null,null,"• Coil Protection ",null,null,null,null,null,"• Low Maintenance"]
[null,null,null,null,"• Protected Compressor",null,null,null,null,null,"• Easy Service Access"]
[null,null,null,null,"• Environmentally Friendly Refrigerant",null,null,null,null,null,"• Secured Service Valves"]
[null,null,null,null,"• Durable Finish",null,null,null,null,null,"• Advanced System Control"]
[null,null,null,null,"• Lower Installed Cost",null,null,null,null,null,"• Agency Listed"]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Extended 10-Years limited parts warranty."]
[null,null,null,null,"• Standard 10-Years limited compressor warranty."]
[null,null,null,null,"• Extended 10-Years limited parts warranty when product is registered online within 90 "]
[null,null,null,null,"   days of purchase for replacement or closing for new home construction."]

{"sheet":"YHJR_YORK_SUMMARY","index":30,"n_rows":45,"n_cols":11,"rows_kept":45,"cut":false,"hidden":true,"merged":[[34,4,34,9],[34,10,34,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[37,4,37,9],[37,10,37,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[45,4,45,12],[41,4,41,12],[40,4,40,12],[42,4,42,12],[43,4,43,12],[44,4,44,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Small Footprint",null,null,null,null,null,"• Top Discharge"]
[null,null,null,null,"• Quality Condenser Coils",null,null,null,null,null,"• Low Operating Sound Level"]
[null,null,null,null,"• Coil Protection",null,null,null,null,null,"• Low Maintenance"]
[null,null,null,null,"• Protected Compressor",null,null,null,null,null,"• Easy Service Access"]
[null,null,null,null,"• Environmentally Friendly Refrigerant",null,null,null,null,null,"• Secured Service Valves"]
[null,null,null,null,"• Durable Finish",null,null,null,null,null,"• Agency Listed"]
[null,null,null,null,"• Lower Installed Cost"]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Standard 5-Years limited parts warranty."]
[null,null,null,null,"• Standard 10-Years limited compressor warranty."]
[null,null,null,null,"• Extended 10-Years limited parts warranty when product is registered online within 90 "]
[null,null,null,null,"   days of purchase for replacement or closing for new home construction."]

{"sheet":"YZF_YORK_SUMMARY","index":31,"n_rows":46,"n_cols":11,"rows_kept":46,"cut":false,"hidden":true,"merged":[[34,4,34,9],[34,10,34,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[40,4,40,9],[40,10,40,12],[43,4,43,12],[37,4,37,9],[38,4,38,9],[37,10,37,12],[39,4,39,9],[39,10,39,12],[38,10,38,12],[44,4,44,12],[45,4,45,12],[46,4,46,12],[42,4,42,12],[41,4,41,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Superior Coil Protection",null,null,null,null,null,"• Composite Base Pan"]
[null,null,null,null,"• Protected Compressor",null,null,null,null,null,"• Isolated Compressor Compartment"]
[null,null,null,null,"• Environmentally Friendly Refrigerant",null,null,null,null,null,"• Lower Installed Cost"]
[null,null,null,null,"• Durable Finish ",null,null,null,null,null,"• Factory Installed Filter-Drier"]
[null,null,null,null,"• Hot Heat Pump",null,null,null,null,null,"• Easy Service Access"]
[null,null,null,null,"• QuietDrive™ System",null,null,null,null,null,"• Communications Capable"]
[null,null,null,null,"• Low RPM Fan Motor",null,null,null,null,null,"• Complete System Control"]
[null,null,null,null,"• Swept Wing Fan",null,null,null,null,null,"• Agency Listed"]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Extended 10-Years limited parts warranty."]
[null,null,null,null,"• Extended Lifetime limited compressor warranty."]
[null,null,null,null,"• Extended parts and compressor warranties require online registration within 90 days"]
[null,null,null,null,"   of purchase for replacement or closing for new home construction."]

{"sheet":"YZH_YORK_SUMMARY","index":32,"n_rows":46,"n_cols":11,"rows_kept":46,"cut":false,"hidden":true,"merged":[[34,4,34,9],[34,10,34,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[40,4,40,9],[40,10,40,12],[37,4,37,9],[37,10,37,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[46,4,46,12],[45,4,45,12],[41,4,41,12],[42,4,42,12],[43,4,43,12],[44,4,44,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Superior Coil Protection",null,null,null,null,null,"• Composite Base Pan"]
[null,null,null,null,"• Protected Compressor",null,null,null,null,null,"• Isolated Compressor Compartment"]
[null,null,null,null,"• Environmentally Friendly Refrigerant",null,null,null,null,null,"• Lower Installed Cost"]
[null,null,null,null,"• Durable Finish ",null,null,null,null,null,"• Factory Installed Filter-Drier"]
[null,null,null,null,"• Hot Heat Pump",null,null,null,null,null,"• Easy Service Access"]
[null,null,null,null,"• QuietDrive™ System",null,null,null,null,null,"• Communications Capable"]
[null,null,null,null,"• Low RPM ECM Fan Motor",null,null,null,null,null,"• Complete System Control"]
[null,null,null,null,"• Swept Wing Fan",null,null,null,null,null,"• Agency Listed"]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Extended 10-Years limited parts warranty. "]
[null,null,null,null,"• Extended Lifetime limited compressor warranty."]
[null,null,null,null,"• Extended parts and compressor warranties require online registration within 90 days"]
[null,null,null,null,"   of purchase for replacement or closing for new home construction."]

{"sheet":"YCJF_YORK_SUMMARY","index":33,"n_rows":45,"n_cols":11,"rows_kept":45,"cut":false,"hidden":true,"merged":[[34,4,34,9],[34,10,34,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[37,4,37,9],[37,10,37,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[45,4,45,12],[41,4,41,12],[40,4,40,12],[42,4,42,12],[43,4,43,12],[44,4,44,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Small Footprint",null,null,null,null,null,"• Top Discharge"]
[null,null,null,null,"• Quality Condenser Coils",null,null,null,null,null,"• Quiet Operation"]
[null,null,null,null,"• Coil Protection",null,null,null,null,null,"• Low Maintenance"]
[null,null,null,null,"• Optional Factory E-Coat",null,null,null,null,null,"• Easy Service Access"]
[null,null,null,null,"• Protected Compressor",null,null,null,null,null,"• Secured Service Valves"]
[null,null,null,null,"• Durable Finish",null,null,null,null,null,"• Agency Listed"]
[null,null,null,null,"• Lower Installed Cost"]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Extended 10-Years limited parts warranty."]
[null,null,null,null,"• Standard 10-Years limited compressor warranty."]
[null,null,null,null,"• Extended 10-Years limited parts warranty requires online registration within 90 days of"]
[null,null,null,null,"   purchase for replacement or closing for new home construction."]

{"sheet":"YZV_YORK_SUMMARY","index":34,"n_rows":45,"n_cols":11,"rows_kept":45,"cut":false,"hidden":true,"merged":[[42,4,42,12],[43,4,43,12],[44,4,44,12],[45,4,45,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[40,4,40,12],[41,4,41,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[37,4,37,9],[37,10,37,12],[34,4,34,9],[34,10,34,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Superior Coil Protection",null,null,null,null,null,"• Composite Base Pan"]
[null,null,null,null,"• Environmentally Friendly Refrigerant",null,null,null,null,null,"• High-Efficiency Outdoor Coil"]
[null,null,null,null,"• Durable Finish",null,null,null,null,null,"• Factory Installed Filter-Drier"]
[null,null,null,null,"• Charge Assurance",null,null,null,null,null,"• Easy Service Access"]
[null,null,null,null,"• QuietDrive™ System",null,null,null,null,null,"• Advanced System Control"]
[null,null,null,null,"• ECM Fan Motor ",null,null,null,null,null,"• Agency Listed"]
[null,null,null,null,"• Swept Wing Fan "]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Extended 10-Years limited parts warranty."]
[null,null,null,null,"• Standard 10-Years limited compressor warranty."]
[null,null,null,null,"• Extended 10-Years limited parts warranty requires online registration within 90 days of"]
[null,null,null,null,"   purchase for replacement or closing for new home construction."]

{"sheet":"YH4_YORK_SUMMARY","index":35,"n_rows":45,"n_cols":11,"rows_kept":45,"cut":false,"hidden":true,"merged":[[42,4,42,12],[43,4,43,12],[44,4,44,12],[45,4,45,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[40,4,40,12],[41,4,41,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[37,4,37,9],[37,10,37,12],[34,4,34,9],[34,10,34,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Easier installation",null,null,null,null,null,"• Low operating sound levels"]
[null,null,null,null,"• Rugged coil protection",null,null,null,null,null,"• Top discharge"]
[null,null,null,null,"• Durable finish",null,null,null,null,null,"• Agency listed"]
[null,null,null,null,"• Protected compressor "]
[null,null,null,null,"• Environmentally friendly"]
[]
[]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Extended 10-Years limited parts warranty."]
[null,null,null,null,"• Standard 10-Years limited compressor warranty."]
[null,null,null,null,"• Extended 10-Years limited parts warranty requires online registration within 90 days of"]
[null,null,null,null,"   purchase for replacement or closing for new home construction."]

{"sheet":"HH8_YORK_SUMMARY","index":36,"n_rows":45,"n_cols":5,"rows_kept":45,"cut":false,"hidden":true,"merged":[[34,4,34,9],[34,10,34,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[37,4,37,9],[37,10,37,12],[42,4,42,12],[43,4,43,12],[44,4,44,12],[45,4,45,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[40,4,40,12],[41,4,41,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• 360 DC inverter driven technology"]
[null,null,null,null,"• Pressure sensor"]
[null,null,null,null,"• Smaller outdoor form factor for"]
[null,null,null,null,"   installation flexibility"]
[null,null,null,null,"• Stable temperature control means"]
[null,null,null,null,"   optimal comfort"]
[null,null,null,null,"• Agency listed"]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Extended 10-Years limited parts warranty."]
[null,null,null,null,"• Standard 10-Years limited compressor warranty."]
[null,null,null,null,"• Extended 10-Years limited parts warranty requires online registration within 90 days of"]
[null,null,null,null,"   purchase for replacement or closing for new home construction."]

{"sheet":"YH6_YORK_SUMMARY","index":37,"n_rows":45,"n_cols":11,"rows_kept":45,"cut":false,"hidden":true,"merged":[[34,4,34,9],[34,10,34,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[37,4,37,9],[37,10,37,12],[42,4,42,12],[43,4,43,12],[44,4,44,12],[45,4,45,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[40,4,40,12],[41,4,41,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Easier installation",null,null,null,null,null,"• Top discharge"]
[null,null,null,null,"• Durable finish",null,null,null,null,null,"• Low operating sound levels"]
[null,null,null,null,"• Rugged coil protection",null,null,null,null,null,"• Agency listed "]
[null,null,null,null,"• Quality Condenser Coils"]
[null,null,null,null,"• Protected compressor "]
[null,null,null,null,"• Environmentally friendly"]
[]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Extended 10-Years limited parts warranty."]
[null,null,null,null,"• Standard 10-Years limited compressor warranty."]
[null,null,null,null,"• Extended 10-Years limited parts warranty requires online registration within 90 days of"]
[null,null,null,null,"   purchase for replacement or closing for new home construction."]

{"sheet":"YH5_YORK_SUMMARY","index":38,"n_rows":45,"n_cols":11,"rows_kept":45,"cut":false,"hidden":true,"merged":[[42,4,42,12],[43,4,43,12],[44,4,44,12],[45,4,45,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[40,4,40,12],[41,4,41,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[37,4,37,9],[37,10,37,12],[34,4,34,9],[34,10,34,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Easier installation",null,null,null,null,null,"• Top discharge"]
[null,null,null,null,"• Durable finish",null,null,null,null,null,"• Low operating sound levels"]
[null,null,null,null,"• Rugged coil protection",null,null,null,null,null,"• Agency listed "]
[null,null,null,null,"• Quality Condenser Coils"]
[null,null,null,null,"• Protected compressor "]
[null,null,null,null,"• Environmentally friendly"]
[]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• Extended 10-Years limited parts warranty."]
[null,null,null,null,"• Standard 10-Years limited compressor warranty."]
[null,null,null,null,"• Extended 10-Years limited parts warranty requires online registration within 90 days of"]
[null,null,null,null,"   purchase for replacement or closing for new home construction."]

{"sheet":"OD_SUMMARY","index":39,"n_rows":50,"n_cols":11,"rows_kept":50,"cut":false,"hidden":true,"merged":[[34,4,34,9],[34,10,34,12],[35,4,35,9],[35,10,35,12],[36,4,36,9],[36,10,36,12],[31,4,31,12],[32,4,32,9],[32,10,32,12],[33,4,33,9],[33,10,33,12],[40,4,40,9],[40,10,40,12],[41,4,41,9],[41,10,41,12],[43,4,43,9],[43,10,43,12],[42,4,42,9],[42,10,42,12],[37,4,37,9],[37,10,37,12],[38,4,38,9],[38,10,38,12],[39,4,39,9],[39,10,39,12],[46,4,46,12],[45,4,45,12],[44,4,44,9],[44,10,44,12],[53,4,53,12],[47,4,47,12],[48,4,48,12],[49,4,49,12],[50,4,50,12],[51,4,51,12],[52,4,52,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• ",null,null,null,null,null,"• "]
[null,null,null,null,"• ",null,null,null,null,null,"• "]
[null,null,null,null,"• ",null,null,null,null,null,"• "]
[null,null,null,null,"• ",null,null,null,null,null,"• "]
[null,null,null,null,"• ",null,null,null,null,null,"• "]
[null,null,null,null,"• ",null,null,null,null,null,"• "]
[null,null,null,null,"• ",null,null,null,null,null,"• "]
[null,null,null,null,"• ",null,null,null,null,null,"• "]
[null,null,null,null,"• ",null,null,null,null,null,"• "]
[null,null,null,null,"• ",null,null,null,null,null,"• "]
[]
[]
[]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• "]
[null,null,null,null,"• "]
[null,null,null,null,"• "]
[null,null,null,null,"     "]

{"sheet":"AM_SUMMARY","index":40,"n_rows":51,"n_cols":10,"rows_kept":51,"cut":false,"hidden":true,"merged":[[36,4,36,12],[37,4,37,12],[38,4,38,12],[39,4,39,12],[51,4,51,12],[48,4,48,12],[40,4,40,12],[41,4,41,12],[42,4,42,12],[44,4,44,12],[43,4,43,12],[45,4,45,12],[46,4,46,12],[47,4,47,12],[49,4,49,12],[50,4,50,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Cabinet constructed of heavy gauge painted steel for additional corrosion resistance."]
[null,null,null,null,"• High quality 5/8\" foil-faced insulation lines cabinet, with cabinet flanges & retaining rods for"]
[null,null,null,null,"better attachment."]
[null,null,null,null,"• Independent lab tested 2% or less air leakage for better efficiency."]
[null,null,null,null,"• Coils are air pressure tested at 500 PSI, leak tested with helium, sealed with rubber plugs, then "]
[null,null,null,null,"charged with dry air."]
[null,null,null,null,"• HYDROTECTM drain pans hold less water, which reduces the possibility of mold and mildew"]
[null,null,null,null,"growing in the pan. "]
[null,null,null,null,"• All drain pans have Microban protection, which inhibits the growth of mold and mildew that"]
[null,null,null,null,"cause odors and staining. "]
[null,null,null,null,"• Fan time delay factory installed (1 second on, 45 seconds off)."]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• AM Series air handlers feature a standard 5-year limited warranty; a 10-year limited warranty is ",null,null,null,null,"Low Maintenance"]
[null,null,null,null,"available with registration."]

{"sheet":"AV_SUMMARY","index":41,"n_rows":52,"n_cols":5,"rows_kept":52,"cut":false,"hidden":true,"merged":[[36,4,36,12],[37,4,37,12],[38,4,38,12],[39,4,39,12],[50,4,50,12],[44,4,44,12],[41,4,41,12],[40,4,40,12],[43,4,43,12],[42,4,42,12],[51,4,51,12],[45,4,45,12],[46,4,46,12],[49,4,49,12],[48,4,48,12],[47,4,47,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Filter rack door with thumb screws for easy access and replacement."]
[null,null,null,null,"• Cabinet constructed of heavy gauge painted steel for additional corrosion resistance."]
[null,null,null,null,"• High quality 5/8\" foil-faced insulation lines cabinet to prevent sweating."]
[null,null,null,null,"• Independent lab tested 2% or less cabinet air leakage for better efficiency."]
[null,null,null,null,"• Coils are air pressure tested at 500 PSI, leak tested with helium, sealed with rubber plugs,"]
[null,null,null,null,"then charged with dry air."]
[null,null,null,null,"• Constant air circulation feature runs airflow at 50% of cooling CFM, improves IAQ and eliminates"]
[null,null,null,null,"stratification."]
[null,null,null,null,"• Soft start feature runs airflow at 82% of cooling CFM for first 7.5 minutes of operation. "]
[null,null,null,null,"• Time delay built into the motor (1 second on; 1 minute off for cooling or HP heating; 2 minutes off"]
[null,null,null,null,"for electric heat or hot water heat)."]
[null,null,null,null,"• Blower door safety switch on all models."]
[null,null,null,null,"• Electric heat kits available for field installation."]
[null,null,null,null,"Warranty "]
[null,null,null,null,"• AV Series air handlers feature a standard 5-year limited warranty."]

{"sheet":"AX_SUMMARY","index":42,"n_rows":51,"n_cols":10,"rows_kept":51,"cut":false,"hidden":true,"merged":[[46,4,46,12],[47,4,47,12],[49,4,49,12],[50,4,50,12],[51,4,51,12],[48,4,48,12],[36,4,36,12],[37,4,37,12],[38,4,38,12],[39,4,39,12],[44,4,44,12],[45,4,45,12],[40,4,40,12],[41,4,41,12],[42,4,42,12],[43,4,43,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[null,null,null,null,"• Cabinet constructed of heavy gauge painted steel for additional corrosion resistance."]
[null,null,null,null,"• High quality 5/8\" foil-faced insulation lines cabinet, with cabinet flanges & retaining rods for"]
[null,null,null,null,"better attachment."]
[null,null,null,null,"• Independent lab tested 2% or less air leakage for better efficiency."]
[null,null,null,null,"• Coils are air pressure tested at 500 PSI, leak tested with helium, sealed with rubber plugs, then "]
[null,null,null,null,"charged with dry air."]
[null,null,null,null,"• HYDROTECTM drain pans hold less water, which reduces the possibility of mold and mildew"]
[null,null,null,null,"growing in the pan. "]
[null,null,null,null,"• All drain pans have Microban protection, which inhibits the growth of mold and mildew that"]
[null,null,null,null,"cause odors and staining. "]
[null,null,null,null,"• Fan time delay factory installed (1 second on, 45 seconds off)."]
[null,null,null,null,"Warranty"]
[null,null,null,null,"• AX Series air handlers feature a standard 5-year limited warranty; a 10-year limited warranty is ",null,null,null,null,"Low Maintenance"]
[null,null,null,null,"available with registration."]

{"sheet":"ID_SUMMARY","index":43,"n_rows":48,"n_cols":5,"rows_kept":48,"cut":false,"hidden":true,"merged":[[48,4,48,12],[50,4,50,12],[47,4,47,12],[36,4,36,12],[37,4,37,12],[38,4,38,12],[39,4,39,12],[40,4,40,12],[41,4,41,12],[42,4,42,12],[44,4,44,12],[45,4,45,12],[46,4,46,12]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Unit Features"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Warranty *"]

{"sheet":"Print","index":44,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}