,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Nominal Cooling Capacity (Tons)##other##,Air Handler Depth##length##inches,Air Handler Width##length##inches,Air Handler Height##length##inches,Case Width##length##inches,Case Depth##length##inches,Case Height##length##inches,Voltage##electrical_potential##volts,Description##other##,Series##other##,Model##other##,Unit Weight Value##number##general,Maximum Air Flow##hvac_air_flow##cubic_feet_per_minute,Minimum Air Flow##hvac_air_flow##cubic_feet_per_minute,Phase##other##,Frequency##electrical_frequency##hertz,Number of Poles##other##,Blower Diameter##length##inches,Blower Width##length##inches,Condensate Drain Connection Diameter##pipe_size##inches,Refrigerant Liquid Connection Diameter##pipe_size##inches,Refrigerant Suction Gas Connection Diameter##pipe_size##inches,Voltage Comments##other##,Supply Air Connection Width##hvac_duct_size##inches,Supply Air Connection Height##hvac_duct_size##inches,Fan Type##Other##,Standards##other##,Supply Air Connection Vertical Offset##length##inches,Drain Pan Offset##length##inches,Coil Housing Depth##length##inches,Case Visibility##other##,URL##other##,Product Page URL##other##
[PSC]-[1.5TON]-[UNCASED]-[CP18],18000,1.5,19.5,37,10.5,39.7,24,11,240,Ceiling-Mount Air Handler,C,CP18,60,680,316,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,30.5,7,PSC,AHRI Certified; ETL Listed,0.75,1,11.25,0,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[PSC]-[1.6TON]-[UNCASED]-[CP19],19000,1.6,19.5,37,10.5,39.7,24,11,240,Ceiling-Mount Air Handler,C,CP19,65,680,316,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,30.5,7,PSC,AHRI Certified; ETL Listed,0.75,1,11.25,0,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[PSC]-[1.9TON]-[UNCASED]-[CP23],23000,1.9,20.5,43,10.5,45.7,24,11,240,Ceiling-Mount Air Handler,C,CP23,63,902,546,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,36.5,7,PSC,AHRI Certified; ETL Listed,0.75,1,11.25,0,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[PSC]-[2TON]-[UNCASED]-[CP24],24000,2,20.5,43,10.5,45.7,24,11,240,Ceiling-Mount Air Handler,C,CP24,65,1039,580,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,36.5,7,PSC,AHRI Certified; ETL Listed,0.75,1,11.25,0,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[PSC]-[2.4TON]-[UNCASED]-[CP29],29000,2.4,20.5,43,10.5,45.7,24,11,240,Ceiling-Mount Air Handler,C,CP29,68,1039,580,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,36.5,7,PSC,AHRI Certified; ETL Listed,0.75,1,11.25,0,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[PSC]-[2.1TON]-[UNCASED]-[CP25],25000,2.1,20.5,49,10.5,51.7,24,11,240,Ceiling-Mount Air Handler,C,CP25,70,1050,553,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,42.5,7,PSC,AHRI Certified; ETL Listed,0.75,1,11.25,0,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[PSC]-[2.5TON]-[UNCASED]-[CP30],30000,2.5,20.5,49,10.5,51.7,24,11,240,Ceiling-Mount Air Handler,C,CP30,70,1050,553,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,42.5,7,PSC,AHRI Certified; ETL Listed,0.75,1,11.25,0,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[ECM]-[1.5TON]-[UNCASED]-[CE18],18000,1.5,19.5,37,10.5,39.7,24,11,240,Ceiling-Mount Air Handler,C,CE18,63,890,301,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,30.5,7,ECM,AHRI Certified; ETL Listed,0.75,1,11.25,0,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[ECM]-[1.6TON]-[UNCASED]-[CE19],19000,1.6,19.5,37,10.5,39.7,24,11,240,Ceiling-Mount Air Handler,C,CE19,68,890,301,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,30.5,7,ECM,AHRI Certified; ETL Listed,0.75,1,11.25,0,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[ECM]-[1.9TON]-[UNCASED]-[CE23],23000,1.9,20.5,43,10.5,45.7,24,11,240,Ceiling-Mount Air Handler,C,CE23,63,937,270,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,36.5,7,ECM,AHRI Certified; ETL Listed,0.75,1,11.25,0,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[ECM]-[2TON]-[UNCASED]-[CE24],24000,2,20.5,43,10.5,45.7,24,11,240,Ceiling-Mount Air Handler,C,CE24,68,937,270,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,36.5,7,ECM,AHRI Certified; ETL Listed,0.75,1,11.25,0,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[ECM]-[2.4TON]-[UNCASED]-[CE29],29000,2.4,20.5,43,10.5,45.7,24,11,240,Ceiling-Mount Air Handler,C,CE29,70,937,270,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,36.5,7,ECM,AHRI Certified; ETL Listed,0.75,1,11.25,0,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[ECM]-[2.1TON]-[UNCASED]-[CE25],25000,2.1,20.5,49,10.5,51.7,24,11,240,Ceiling-Mount Air Handler,C,CE25,73,984,277,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,42.5,7,ECM,AHRI Certified; ETL Listed,0.75,1,11.25,0,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[ECM]-[2.5TON]-[UNCASED]-[CE30],30000,2.5,20.5,49,10.5,51.7,24,11,240,Ceiling-Mount Air Handler,C,CE30,73,984,277,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,42.5,7,ECM,AHRI Certified; ETL Listed,0.75,1,11.25,0,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[PSC]-[1.5TON]-[CASED]-[CP18],18000,1.5,19.5,37,10.5,39.7,24,11,240,Ceiling-Mount Air Handler,C,CP18,89,680,316,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,30.5,7,PSC,AHRI Certified; ETL Listed,0.75,1,11.25,1,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[PSC]-[1.6TON]-[CASED]-[CP19],19000,1.6,19.5,37,10.5,39.7,24,11,240,Ceiling-Mount Air Handler,C,CP19,97,680,316,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,30.5,7,PSC,AHRI Certified; ETL Listed,0.75,1,11.25,1,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[PSC]-[1.9TON]-[CASED]-[CP23],23000,1.9,20.5,43,10.5,45.7,24,11,240,Ceiling-Mount Air Handler,C,CP23,92,902,546,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,36.5,7,PSC,AHRI Certified; ETL Listed,0.75,1,11.25,1,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[PSC]-[2TON]-[CASED]-[CP24],24000,2,20.5,43,10.5,45.7,24,11,240,Ceiling-Mount Air Handler,C,CP24,97,1039,580,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,36.5,7,PSC,AHRI Certified; ETL Listed,0.75,1,11.25,1,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[PSC]-[2.4TON]-[CASED]-[CP29],29000,2.4,20.5,43,10.5,45.7,24,11,240,Ceiling-Mount Air Handler,C,CP29,103,1039,580,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,36.5,7,PSC,AHRI Certified; ETL Listed,0.75,1,11.25,1,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[PSC]-[2.1TON]-[CASED]-[CP25],25000,2.1,20.5,49,10.5,51.7,24,11,240,Ceiling-Mount Air Handler,C,CP25,105,1050,553,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,42.5,7,PSC,AHRI Certified; ETL Listed,0.75,1,11.25,1,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[PSC]-[2.5TON]-[CASED]-[CP30],30000,2.5,20.5,49,10.5,51.7,24,11,240,Ceiling-Mount Air Handler,C,CP30,105,1050,553,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,42.5,7,PSC,AHRI Certified; ETL Listed,0.75,1,11.25,1,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[ECM]-[1.5TON]-[CASED]-[CE18],18000,1.5,19.5,37,10.5,39.7,24,11,240,Ceiling-Mount Air Handler,C,CE18,92,890,301,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,30.5,7,ECM,AHRI Certified; ETL Listed,0.75,1,11.25,1,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[ECM]-[1.6TON]-[CASED]-[CE19],19000,1.6,19.5,37,10.5,39.7,24,11,240,Ceiling-Mount Air Handler,C,CE19,100,890,301,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,30.5,7,ECM,AHRI Certified; ETL Listed,0.75,1,11.25,1,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[ECM]-[1.9TON]-[CASED]-[CE23],23000,1.9,20.5,43,10.5,45.7,24,11,240,Ceiling-Mount Air Handler,C,CE23,92,937,270,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,36.5,7,ECM,AHRI Certified; ETL Listed,0.75,1,11.25,1,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[ECM]-[2TON]-[CASED]-[CE24],24000,2,20.5,43,10.5,45.7,24,11,240,Ceiling-Mount Air Handler,C,CE24,100,937,270,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,36.5,7,ECM,AHRI Certified; ETL Listed,0.75,1,11.25,1,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[ECM]-[2.4TON]-[CASED]-[CE29],29000,2.4,20.5,43,10.5,45.7,24,11,240,Ceiling-Mount Air Handler,C,CE29,105,937,270,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,36.5,7,ECM,AHRI Certified; ETL Listed,0.75,1,11.25,1,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[ECM]-[2.1TON]-[CASED]-[CE25],25000,2.1,20.5,49,10.5,51.7,24,11,240,Ceiling-Mount Air Handler,C,CE25,108,984,277,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,42.5,7,ECM,AHRI Certified; ETL Listed,0.75,1,11.25,1,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
[ECM]-[2.5TON]-[CASED]-[CE30],30000,2.5,20.5,49,10.5,51.7,24,11,240,Ceiling-Mount Air Handler,C,CE30,108,984,277,1,60,1,5.75,6.75,0.75,0.375,0.75,208 VAC - 230 VAC,42.5,7,ECM,AHRI Certified; ETL Listed,0.75,1,11.25,1,https://www.adpnow.com/,https://www.adpnow.com/product/soffit-mount-cp-series/
